## Phidget Resistance Input.lvlib:ResistanceInputSetDataInterval.vi

The `ResistanceInputDataInterval` is the time that must elapse before the channel will fire another `ResistanceInput_ResistanceChange` event.

- The data interval is bounded by `ResistanceInputMinDataInterval` and `ResistanceInputMaxDataInterval`.
- The timing between `ResistanceInput_ResistanceChange` events can also be affected by the `ResistanceInputResistanceChangeTrigger`.

| Device In Device # Identification

| error in (no error) error in can accept error information wired from VIs previously called.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Interval The data interval value Units: milliseconds (ms) TMP1200_0 (ver: 104, 105, 106, 107, 108, 109, 110) Resistance Input: Min: 250 Max: 60000 Default: 250 TMP1200_1 (ver: 300, 301, 302) Resistance Input: Min: 333 Max: 60000 Default: 333

| Device Out Same as Device In

| error out error out passes error or warning information out of a VI to be used by other VIs.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.