## Phidget Voltage Input.lvlib:VoltageInputGetSensorValue.vi

The most recent sensor value that the channel has reported.

- Use `VoltageInputSensorUnit` to get the measurement units that are associated with the `VoltageInputSensorValue`

| Device In Device # Identification

| error in (no error) error in can accept error information wired from VIs previously called.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Device Out Same as Device In

| error out error out passes error or warning information out of a VI to be used by other VIs.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Sensor Value The sensor value 1010_0 (ver: 903, 904) Voltage Input: 1011_0 (ver: 100, 101, 102, 103) Voltage Input: 1013_0 (ver: 800, 811, 820) Voltage Input: 1013_0 (ver: 821, 823) Voltage Input: 1018_0 (ver: 824, 825, 826) Voltage Input: 1018_1 (ver: 826) Voltage Input: 1018_2 (ver: 900, 901, 902, 903, 904) Voltage Input: 1018_3 (ver: 1000, 1001) Voltage Input: 1019_0 (ver: 826) Voltage Input: 1019_1 (ver: 903, 904) Voltage Input: 1065_0 (ver: 100, 101) Voltage Input: 1065_1 (ver: 100, 101) Voltage Input: 1070_0 (ver: 826) Voltage Input: 1072_0 (ver: 903) Voltage Input: 1073_0 (ver: 904) Voltage Input: 1202_0 (ver: 100) Voltage Input: 1202_0 (ver: 120, 121) Voltage Input: 1202_1 (ver: 123, 124) Voltage Input: 1202_2 (ver: 200, 201, 202, 203, 204) Voltage Input: 1203_0 (ver: 100) Voltage Input: 1203_0 (ver: 120, 121) Voltage Input: 1203_1 (ver: 123, 124) Voltage Input: 1203_2 (ver: 200, 201, 202, 203, 204) Voltage Input: ADP1000_0 (ver: 104, 105) Voltage Input: DAQ1000_0 (ver: 102, 103) Voltage Input: DAQ1000_0 (ver: 110, 111, 112, 114) Voltage Input: DAQ1400_0 (ver: 112) Voltage Input: DAQ1400_0 (ver: 120, 121) Voltage Input: DAQ1400_0 (ver: 130) Voltage Input: HUB0000_0 (ver: 117, 118, 119) Voltage Input: HUB0000_0 (ver: 121, 125, 126, 127) Voltage Input: HUB0000_0 (ver: 307) Voltage Input: HUB0000_1 (ver: 400, 401) Voltage Input: HUB0001_0 (ver: 111, 113, 114) Voltage Input: HUB0001_0 (ver: 115, 116) Voltage Input: HUB0002_0 (ver: 100, 101) Voltage Input: HUB0007_0 (ver: 101, 102) Voltage Input: HUB5000_0 (ver: 100) Voltage Input: HUB5000_0 (ver: 102, 104, 105, 106) Voltage Input: HUB5000_0 (ver: 107) Voltage Input: HUB5000_0 (ver: 203, 204, 205) Voltage Input: SBC3003_0 (ver: 101, 102) Voltage Input: SBC3003_0 (ver: 108, 109, 110) Voltage Input: SBC3003_0 (ver: 203, 204) Voltage Input: