## Phidget Voltage Input.lvlib:VoltageInputSetVoltageRange.vi

The voltage range you choose should allow you to measure the full range of your input signal.

- A larger `VoltageInputVoltageRange` equates to less resolution.
- If a `VoltageInputSaturation` event occurs, increase the voltage range.

| Device In Device # Identification

| error in (no error) error in can accept error information wired from VIs previously called.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Voltage Range The voltage range value
Enumeration Values
Name | Value | Supported Devices
--- | --- | ---
ADP1000_0 v104 v105 | VCP1000_0 v100 v101 | VCP1001_0 v100 | VCP1001_0 v110 | VCP1002_0 v106 | VCP1002_0 v110
VOLTAGE_RANGE_10mV | 1 | X | X | X | X | ✓ | ✓
VOLTAGE_RANGE_40mV | 2 | X | X | X | X | ✓ | ✓
VOLTAGE_RANGE_200mV | 3 | X | X | X | X | ✓ | ✓
VOLTAGE_RANGE_312_5mV | 4 | X | ✓ | X | X | X | X
VOLTAGE_RANGE_400mV | 5 | ✓ | X | X | X | X | X
VOLTAGE_RANGE_1000mV | 6 | X | X | X | X | ✓ | ✓
VOLTAGE_RANGE_2V | 7 | ✓ | X | X | X | X | X
VOLTAGE_RANGE_5V | 8 | X | X | ✓ | ✓ | X | X
VOLTAGE_RANGE_15V | 9 | X | X | ✓ | ✓ | X | X
VOLTAGE_RANGE_40V | 10 | X | ✓ | ✓ | ✓ | X | X
VOLTAGE_RANGE_AUTO | 11 | X | X | ✓ | ✓ | ✓ | ✓
ADP1000_0 (ver: 104, 105) Voltage Input: Default: VOLTAGE_RANGE_400mV VCP1000_0 (ver: 100, 101) Voltage Input: Default: VOLTAGE_RANGE_40V VCP1001_0 (ver: 100) Voltage Input: Default: VOLTAGE_RANGE_AUTO VCP1001_0 (ver: 110) Voltage Input: Default: VOLTAGE_RANGE_AUTO VCP1002_0 (ver: 106) Voltage Input: Default: VOLTAGE_RANGE_AUTO VCP1002_0 (ver: 110) Voltage Input: Default: VOLTAGE_RANGE_AUTO

| Device Out Same as Device In

| error out error out passes error or warning information out of a VI to be used by other VIs.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.