## Phidget Voltage Ratio Input.lvlib:VoltageRatioInputSetBridgeGain.vi

Choose a `VoltageRatioInputBridgeGain` that best suits your application.

- For more information about the range and accuracy of each `VoltageRatioInputBridgeGain` to decide which best suits your application, see your device's User Guide.

| Device In Device # Identification

| error in (no error) error in can accept error information wired from VIs previously called.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Bridge Gain The bridge gain value
Enumeration Values
Name | Value | Supported Devices
--- | --- | ---
1046_0 v100 v101 | 1046_0 v102 | 1046_1 v200 v201 | DAQ1500_0 v104
BRIDGE_GAIN_1 | 1 | ✓ | ✓ | ✓ | ✓
BRIDGE_GAIN_2 | 2 | X | X | X | ✓
BRIDGE_GAIN_4 | 3 | X | X | X | X
BRIDGE_GAIN_8 | 4 | ✓ | ✓ | ✓ | X
BRIDGE_GAIN_16 | 5 | ✓ | ✓ | ✓ | X
BRIDGE_GAIN_32 | 6 | ✓ | ✓ | ✓ | X
BRIDGE_GAIN_64 | 7 | ✓ | ✓ | ✓ | ✓
BRIDGE_GAIN_128 | 8 | ✓ | ✓ | ✓ | ✓
1046_0 (ver: 100, 101) Bridge Input: Default: BRIDGE_GAIN_128 1046_0 (ver: 102) Bridge Input: Default: BRIDGE_GAIN_128 1046_1 (ver: 200, 201) Bridge Input: Default: BRIDGE_GAIN_128 DAQ1500_0 (ver: 104) Bridge Input: Default: BRIDGE_GAIN_128

| Device Out Same as Device In

| error out error out passes error or warning information out of a VI to be used by other VIs.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.