## Phidget Temperature Sensor.lvlib:TemperatureEventExe.vi

The most recent temperature value the channel has measured will be reported in this event, which occurs when the `TemperatureSensorDataInterval` has elapsed.

- If a `TemperatureSensorTemperatureChangeTrigger` has been set to a non-zero value, the `TemperatureSensor_TemperatureChange` event will not occur until the temperature has changed by at least the `TemperatureSensorTemperatureChangeTrigger` value.

Device Support:

1045_0 (ver: 100, 101) Temperature Sensor (IR) : Supported

1045_0 (ver: 100, 101) Temperature Sensor (IC) : Supported

1045_1 (ver: 101) Temperature Sensor (IR) : Supported

1045_1 (ver: 101) Temperature Sensor (IC) : Supported

1048_0 (ver: 100, 101, 102) Thermocouple Input : Supported

1048_0 (ver: 100, 101, 102) Temperature Sensor (IC) : Supported

1048_1 (ver: 200, 202, 204, 205) Thermocouple Input : Supported

1048_1 (ver: 200, 202, 204, 205) Temperature Sensor (IC) : Supported

1048_2 (ver: 210, 212, 214, 215) Thermocouple Input : Supported

1048_2 (ver: 210, 212, 214, 215) Temperature Sensor (IC) : Supported

1051_0 (ver: 100) Thermocouple Input : Supported

1051_0 (ver: 100) Temperature Sensor (IC) : Supported

1051_0 (ver: 200, 201, 202) Thermocouple Input : Supported

1051_0 (ver: 200, 201, 202) Temperature Sensor (IC) : Supported

1051_1 (ver: 300) Thermocouple Input : Supported

1051_1 (ver: 300) Temperature Sensor (IC) : Supported

1051_2 (ver: 400, 401, 402) Thermocouple Input : Supported

1051_2 (ver: 400, 401, 402) Temperature Sensor (IC) : Supported

DCC1000_0 (ver: 115) Temperature Sensor : Supported

DCC1000_0 (ver: 204, 205, 206) Temperature Sensor : Supported

DCC1000_0 (ver: 210, 211, 220) Temperature Sensor : Supported

DCC1020_0 (ver: 103) Temperature Sensor : Supported

DCC1100_0 (ver: 113, 114) Temperature Sensor : Supported

DCC1100_0 (ver: 120, 121, 130) Temperature Sensor : Supported

DCC1120_0 (ver: 104) Temperature Sensor : Supported

HUM1000_0 (ver: 104, 105) Temperature Sensor : Supported

HUM1001_0 (ver: 102) Temperature Sensor : Supported

MOT0109_0 (ver: 112, 113, 115, 117) Temperature Sensor : Supported

MOT0110_0 (ver: 100, 104, 110) Temperature Sensor : Supported

MOT0110_0 (ver: 100, 104, 110) Temperature Sensor : Supported

SAF1000_0 (ver: 101, 102) Temperature Sensor : Supported

SAF1000_0 (ver: 110, 120) Temperature Sensor : Supported

TMP1000_0 (ver: 105, 107) Temperature Sensor (IC) : Supported

TMP1100_0 (ver: 103, 105, 106, 108, 109, 110) Thermocouple Input : Supported

TMP1100_0 (ver: 103, 105, 106, 108, 109, 110) Temperature Sensor (IC) : Supported

TMP1101_0 (ver: 104, 106, 107, 109, 110) Thermocouple Input : Supported

TMP1101_0 (ver: 104, 106, 107, 109, 110) Temperature Sensor (IC) : Supported

TMP1101_1 (ver: 201, 202, 203, 204, 205) Thermocouple Input : Supported

TMP1101_1 (ver: 201, 202, 203, 204, 205) Temperature Sensor (IC) : Supported

TMP1200_0 (ver: 104, 105, 106, 107, 108, 109, 110) RTD input : Supported

TMP1200_1 (ver: 300, 301, 302) RTD input : Supported

| error in (no error) error in can accept error information wired from VIs previously called.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Devices In A list of devices registered for the same type of event

| Device In Device # Identification

| Event Registration Refnum In Event # Identification

| error out error out passes error or warning information out of a VI to be used by other VIs.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error out indicator on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error out indicator on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source string describes the origin of the error or warning. Right-click the error out indicator on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Event? Returns TRUE if the event has executed, or FALSE otherwise.

| Devices Out Same as Devices In

| Device Out Same as Device In

| Index The index of the device that triggered the event within the Devices In array.

| Temperature The temperature

| Event Registration Refnum Out Same as Event Registration Refnum In