## Phidget Encoder.lvlib:EncoderGetMinDataInterval.vi

The minimum value that `EncoderDataInterval` can be set to.

| Device In Device # Identification

| error in (no error) error in can accept error information wired from VIs previously called.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Device Out Same as Device In

| error out error out passes error or warning information out of a VI to be used by other VIs.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Min Data Interval The data interval value Units: milliseconds (ms) 1047_0 (ver: 100, 101, 102) Encoder Input: Constant: 8 1047_1 (ver: 102, 103) Encoder Input: Constant: 8 1047_2 (ver: 200) Encoder Input: Constant: 8 1047_2 (ver: 301) Encoder Input: Constant: 8 1052_0 (ver: 100) Encoder Input: Constant: 16 1052_0 (ver: 101, 102, 103) Encoder Input: Constant: 16 1052_0 (ver: 110, 111) Encoder Input: Constant: 16 1057_0 (ver: 300, 301) Encoder Input: Constant: 8 1057_1 (ver: 302) Encoder Input: Constant: 8 1057_2 (ver: 302) Encoder Input: Constant: 8 1057_3 (ver: 400, 401) Encoder Input: Constant: 8 1065_0 (ver: 100, 101) Encoder Input: Constant: 8 1065_1 (ver: 100, 101) Encoder Input: Constant: 8 DCC1000_0 (ver: 115) Encoder Input: Constant: 100 DCC1000_0 (ver: 204, 205, 206) Encoder Input: Constant: 100 DCC1000_0 (ver: 210, 211, 220) Encoder Input: Constant: 100 DCC1001_0 (ver: 114, 116, 117) Encoder Input: Constant: 50 DCC1001_0 (ver: 120, 130) Encoder Input: Constant: 50 DCC1002_0 (ver: 100, 101, 102) Encoder Input: Constant: 50 DCC1002_0 (ver: 111, 120) Encoder Input: Constant: 50 DCC1020_0 (ver: 103) Encoder Input: Constant: 1 DCC1120_0 (ver: 104) Encoder Input: Constant: 1 ENC1000_0 (ver: 101) Encoder Input: Constant: 20 ENC1001_0 (ver: 100) Encoder Input: Constant: 1 HIN1101_0 (ver: 101) Encoder Input: Constant: 20