## Phidget Motor Position Controller.lvlib:MotorPositionControllerPositionChangeEventExe.vi

The most recent position value will be reported in this event, which occurs when the `MotorPositionControllerDataInterval` has elapsed.

- Regardless of the `MotorPositionControllerDataInterval`, this event will occur only when the position value has changed from the previous value reported.
- Use the `MotorPositionControllerRescaleFactor` to convert the units of this property to more intuitive units, such as rotations or degrees.

Device Support:

DCC1000_0 (ver: 204, 205, 206) Position Controller : Supported

DCC1000_0 (ver: 210, 211, 220) Position Controller : Supported

DCC1001_0 (ver: 114, 116, 117) Position Controller : Supported

DCC1001_0 (ver: 120, 130) Position Controller : Supported

DCC1002_0 (ver: 100, 101, 102) Position Controller : Supported

DCC1002_0 (ver: 111, 120) Position Controller : Supported

DCC1020_0 (ver: 103) Position Controller : Supported

DCC1100_0 (ver: 113, 114) Position Controller : Supported

DCC1100_0 (ver: 120, 121, 130) Position Controller : Supported

DCC1120_0 (ver: 104) Position Controller : Supported

| error in (no error) error in can accept error information wired from VIs previously called.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Devices In A list of devices registered for the same type of event

| Device In Device # Identification

| Event Registration Refnum In Event # Identification

| error out error out passes error or warning information out of a VI to be used by other VIs.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error out indicator on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error out indicator on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source string describes the origin of the error or warning. Right-click the error out indicator on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Event? Returns TRUE if the event has executed, or FALSE otherwise.

| Devices Out Same as Devices In

| Device Out Same as Device In

| Index The index of the device that triggered the event within the Devices In array.

| phid Device # Identification of the device that triggered the event.

| Position The position value

| Event Registration Refnum Event # Identification