## Phidget Capacitive Touch.lvlib:CapacitiveTouchSetTrigger.vi

The channel will not issue a `CapacitiveTouch_Touch` event until the touch value has changed by the amount specified by the `CapacitiveTouchTouchValueChangeTrigger`.

- Setting the `CapacitiveTouchTouchValueChangeTrigger` to 0 will result in the channel firing events every `CapacitiveTouchDataInterval`. This is useful for applications that implement their own data filtering

| Device In Device # Identification

| error in (no error) error in can accept error information wired from VIs previously called.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Trigger The change trigger value 1015_0 (ver: 500, 101, 102) Capacitive Slider Sensor: Min: 0 Max: 1 Default: 0.005 1016_0 (ver: 510, 101, 102) Capacitive Scroll Sensor: Min: 0 Max: 1 Default: 0.005 HIN1000_0 (ver: 104) Capacitive Touch Sensor: Min: 0 Max: 1 Default: 0 HIN1001_0 (ver: 103) Capacitive Touch Sensor: Min: 0 Max: 0.5 Default: 0 HIN1001_0 (ver: 103) Capacitive Scroll Wheel: Min: 0 Max: 0.5 Default: 0

| Device Out Same as Device In

| error out error out passes error or warning information out of a VI to be used by other VIs.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.