## Phidget Resistance Input.lvlib:ResistanceInputGetResistance.vi

The most recent resistance value that the channel has reported.

- This value will always be between `ResistanceInputMinResistance` and `ResistanceInputMaxResistance`.
- The `ResistanceInputResistance` value will change when the device is also being used as a temperature sensor. This is a side effect of increasing accuracy on the temperature channel.

| Device In Device # Identification

| error in (no error) error in can accept error information wired from VIs previously called.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Device Out Same as Device In

| error out error out passes error or warning information out of a VI to be used by other VIs.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Resistance The resistance value Units: ohms (Ω) TMP1200_0 (ver: 104, 105, 106, 107, 108, 109, 110) Resistance Input: Min: 0 Max: 50000 TMP1200_1 (ver: 300, 301, 302) Resistance Input: Min: 0 Max: 5000