## Phidget Voltage Ratio Input.lvlib:VoltageRatioInputSetSensorTrigger.vi

The channel will not issue a `VoltageRatioInput_SensorChange` event until the sensor value has changed by the amount specified by the `VoltageRatioInputSensorValueChangeTrigger`.

- Setting the `VoltageRatioInputSensorValueChangeTrigger` to 0 will result in the channel firing events every `VoltageRatioInputDataInterval`. This is useful for applications that implement their own data filtering

| Device In Device # Identification

| error in (no error) error in can accept error information wired from VIs previously called.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Trigger The change trigger value 1010_0 (ver: 903, 904) Voltage Ratio Input: Default: 0 1011_0 (ver: 100, 101, 102, 103) Voltage Ratio Input: Default: 0 1013_0 (ver: 800, 811, 820) Voltage Ratio Input: Default: 0 1013_0 (ver: 821, 823) Voltage Ratio Input: Default: 0 1018_0 (ver: 824, 825, 826) Voltage Ratio Input: Default: 0 1018_1 (ver: 826) Voltage Ratio Input: Default: 0 1018_2 (ver: 900, 901, 902, 903, 904) Voltage Ratio Input: Default: 0 1018_3 (ver: 1000, 1001) Voltage Ratio Input: Default: 0 1019_0 (ver: 826) Voltage Ratio Input: Default: 0 1019_1 (ver: 903, 904) Voltage Ratio Input: Default: 0 1065_0 (ver: 100, 101) Voltage Ratio Input: Default: 0 1065_1 (ver: 100, 101) Voltage Ratio Input: Default: 0 1070_0 (ver: 826) Voltage Ratio Input: Default: 0 1072_0 (ver: 903) Voltage Ratio Input: Default: 0 1073_0 (ver: 904) Voltage Ratio Input: Default: 0 1202_0 (ver: 100) Voltage Ratio Input: Default: 0 1202_0 (ver: 120, 121) Voltage Ratio Input: Default: 0 1202_1 (ver: 123, 124) Voltage Ratio Input: Default: 0 1202_2 (ver: 200, 201, 202, 203, 204) Voltage Ratio Input: Default: 0 1203_0 (ver: 100) Voltage Ratio Input: Default: 0 1203_0 (ver: 120, 121) Voltage Ratio Input: Default: 0 1203_1 (ver: 123, 124) Voltage Ratio Input: Default: 0 1203_2 (ver: 200, 201, 202, 203, 204) Voltage Ratio Input: Default: 0 DAQ1000_0 (ver: 102, 103) Voltage Ratio Input: Default: 0 DAQ1000_0 (ver: 110, 111, 112, 114) Voltage Ratio Input: Default: 0 DCC1000_0 (ver: 115) Voltage Ratio: Default: 0 DCC1000_0 (ver: 204, 205, 206) Voltage Ratio: Default: 0 DCC1000_0 (ver: 210, 211, 220) Voltage Ratio: Default: 0 HUB0000_0 (ver: 117, 118, 119) Voltage Ratio Input: Default: 0 HUB0000_0 (ver: 121, 125, 126, 127) Voltage Ratio Input: Default: 0 HUB0000_0 (ver: 307) Voltage Ratio Input: Default: 0 HUB0000_1 (ver: 400, 401) Voltage Ratio Input: Default: 0 HUB0001_0 (ver: 111, 113, 114) Voltage Ratio Input: Default: 0 HUB0001_0 (ver: 115, 116) Voltage Ratio Input: Default: 0 HUB0002_0 (ver: 100, 101) Voltage Ratio Input: Default: 0 HUB0007_0 (ver: 101, 102) Voltage Ratio Input: Default: 0 HUB5000_0 (ver: 100) Voltage Ratio Input: Default: 0 HUB5000_0 (ver: 102, 104, 105, 106) Voltage Ratio Input: Default: 0 HUB5000_0 (ver: 107) Voltage Ratio Input: Default: 0 HUB5000_0 (ver: 203, 204, 205) Voltage Ratio Input: Default: 0 SBC3003_0 (ver: 101, 102) Voltage Ratio Input: Default: 0 SBC3003_0 (ver: 108, 109, 110) Voltage Ratio Input: Default: 0 SBC3003_0 (ver: 203, 204) Voltage Ratio Input: Default: 0

| Device Out Same as Device In

| error out error out passes error or warning information out of a VI to be used by other VIs.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.