## Phidget LCD.lvlib:LCDWriteText.vi

Writes text to the current frame buffer at the specified location

- Changes made to the frame buffer must be flushed to the LCD screen using `LCDFlush`.

Device Support:

1202_0 (ver: 100) Text LCD : Supported

1202_0 (ver: 120, 121) Text LCD : Supported

1202_1 (ver: 123, 124) Text LCD : Supported

1202_2 (ver: 200, 201, 202, 203, 204) Text LCD : Supported

1203_0 (ver: 100) Text LCD : Supported

1203_0 (ver: 120, 121) Text LCD : Supported

1203_1 (ver: 123, 124) Text LCD : Supported

1203_2 (ver: 200, 201, 202, 203, 204) Text LCD : Supported

1204_0 (ver: 100, 101) Text LCD : Supported

1215_0 (ver: 100, 101) Text LCD : Supported

1216_0 (ver: 100, 101) Text LCD : Supported

1217_0 (ver: 100, 101) Text LCD : Supported

1218_0 (ver: 100, 101) Text LCD : Supported

1219_0 (ver: 110, 111, 113) Text LCD : Supported

1220_0 (ver: 110, 111, 113) Text LCD : Supported

1221_0 (ver: 110, 111, 113) Text LCD : Supported

1222_0 (ver: 110, 111, 113) Text LCD : Supported

LCD1100_0 (ver: 106, 107, 108, 110) Graphic LCD : Supported

LCD1100_1 (ver: 200, 201, 202) Graphic LCD : Supported

| Device In Device # Identification

| error in (no error) error in can accept error information wired from VIs previously called.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Text The text to be written

| xpos The X position of the start of the text string

| ypos The Y position of the start of the text string

| Font The font the character belongs to
Enumeration Values
Name | Value | Supported Devices
--- | --- | ---
1202_0 v100 | 1202_0 v120 v121 | 1202_1 v123 v124 | 1202_2 v200 v201 v202 v203 v204 | 1203_0 v100 | 1203_0 v120 v121 | 1203_1 v123 v124 | 1203_2 v200 v201 v202 v203 v204 | 1204_0 v100 v101 | 1215_0 v100 v101 | 1216_0 v100 v101 | 1217_0 v100 v101 | 1218_0 v100 v101 | 1219_0 v110 v111 v113 | 1220_0 v110 v111 v113 | 1221_0 v110 v111 v113 | 1222_0 v110 v111 v113 | LCD1100_0 v106 v107 v108 v110 | LCD1100_1 v200 v201 v202
FONT_User1 | 1 | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | ✓ | ✓
FONT_User2 | 2 | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | ✓ | ✓
FONT_6x10 | 3 | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | ✓ | ✓
FONT_5x8 | 4 | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓
FONT_6x12 | 5 | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | ✓ | ✓

| Device Out Same as Device In

| error out error out passes error or warning information out of a VI to be used by other VIs.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.