## Phidget RFID.lvlib:RFID_TagEventExe.vi

Occurs when an RFID tag is read.

Device Support:

1023_0 (ver: 103) RFID Reader : Supported

1023_0 (ver: 104) RFID Reader : Supported

1023_0 (ver: 200) RFID Reader : Supported

1023_0 (ver: 201, 202, 203, 204) RFID Reader : Supported

1023_1 (ver: 205, 206) RFID Reader : Supported

1024_0 (ver: 100, 101, 103) RFID Reader/Writer : Supported

1024_1 (ver: 301) RFID Reader/Writer : Supported

1024_1 (ver: 301) RFID Reader/Writer : Supported

1024_1 (ver: 310) RFID Reader/Writer : Supported

1024_1 (ver: 310) RFID Reader/Writer : Supported

1024_1 (ver: 320) RFID Reader/Writer : Supported

1024_1 (ver: 320) RFID Reader/Writer : Supported

| error in (no error) error in can accept error information wired from VIs previously called.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Devices In A list of devices registered for the same type of event

| Device In Device # Identification

| Event Registration Refnum In Event # Identification

| error out error out passes error or warning information out of a VI to be used by other VIs.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error out indicator on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error out indicator on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source string describes the origin of the error or warning. Right-click the error out indicator on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Event? Returns TRUE if the event has executed, or FALSE otherwise.

| Devices Out Same as Devices In

| Device Out Same as Device In

| Index The index of the device that triggered the event within the Devices In array.

| phid Device # Identification of the device that triggered the event.

| Tag String Data from the tag

| Event Registration Refnum Out Same as Event Registration Refnum In

| Protocol Communication protocol of the tag
Enumeration Values
Name | Value | Supported Devices
--- | --- | ---
1023_0 v103 | 1023_0 v104 | 1023_0 v200 | 1023_0 v201 v202 v203 v204 | 1023_1 v205 v206 | 1024_0 v100 v101 v103 | 1024_1 v301 | 1024_1 v301 | 1024_1 v310 | 1024_1 v310 | 1024_1 v320 | 1024_1 v320
PROTOCOL_EM4100 | 1 | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓
PROTOCOL_ISO11785_FDX_B | 2 | X | X | X | X | X | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓
PROTOCOL_PHIDGETS | 3 | X | X | X | X | X | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓
PROTOCOL_HID_GENERIC | 4 | X | X | X | X | X | X | X | X | ✓ | ✓ | ✓ | ✓
PROTOCOL_HID_H10301 | 5 | X | X | X | X | X | X | X | X | ✓ | ✓ | ✓ | ✓
PROTOCOL_NFC | 6 | X | X | X | X | X | X | X | X | X | X | X | X