## Phidget Motor Velocity Controller.lvlib:MotorVelocityControllerGetActiveCurrentLimit.vi

The current limit that the controller is actively following. The `MotorVelocityControllerSurgeCurrentLimit`, `MotorVelocityControllerCurrentLimit`, and temperature will impact this value.

| Device In Device # Identification

| error in (no error) error in can accept error information wired from VIs previously called.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Device Out Same as Device In

| error out error out passes error or warning information out of a VI to be used by other VIs.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Active Current Limit The active current limit value Units: amperes (A) DCC1020_0 (ver: 103, 104) Velocity Controller: DCC1030_0 (ver: 104) Velocity Controller: DCC1120_0 (ver: 104, 105) Velocity Controller: DCC1130_0 (ver: 105) Velocity Controller: