## Phidget Sound Sensor.lvlib:SoundSensorStart.vi

Opens and initializes a Phidget Sound Sensor

| Change Trigger The change trigger value Units: sound pressure level (dB SPL) SND1000_0 (ver: 101, 102) Sound Sensor: Min: 0 Max: 102 Default: 0 SND1000_1 (ver: 102) Sound Sensor: Min: 0 Max: 102 Default: 0

| Data Interval The data interval value Units: milliseconds (ms) SND1000_0 (ver: 101, 102) Sound Sensor: Min: 100 Max: 60000 Default: 250 SND1000_1 (ver: 102) Sound Sensor: Min: 100 Max: 60000 Default: 250

| error in (no error) error in can accept error information wired from VIs previously called.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Device Info Information required to specify which Phidget to open

| Serial Number The device serial number

| Channel The channel index

| Port The hub port index

| Connection Selects whether to look for a Phidget on the Local machine, over a Remote network, or both (No Preference)

| Timeout (mSec) Timeout in milliseconds

| SPL Range The range value.
Enumeration Values
Name | Value | Supported Devices
--- | --- | ---
SND1000_0 v101 v102 | SND1000_1 v102
SPL_RANGE_102dB | 1 | ✓ | ✓
SPL_RANGE_82dB | 2 | ✓ | ✓
SND1000_0 (ver: 101, 102) Sound Sensor: Default: SPL_RANGE_102dB SND1000_1 (ver: 102) Sound Sensor: Default: SPL_RANGE_102dB

| Attached? Returns TRUE is the device successfully attached, or FALSE otherwise

| error out error out passes error or warning information out of a VI to be used by other VIs.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Phidget ID Device # Identification

| Serial Number Return The device serial number