## Phidget Motor Velocity Controller.lvlib:MotorVelocityControllerSetDeadBand.vi

This parameter specifies a minimum `MotorVelocityControllerVelocity` below which your system will relax if the `MotorVelocityControllerTargetVelocity` is set to 0, to prevent unwanted jitter.

- Use the `MotorVelocityControllerRescaleFactor` to convert the units of this property to more intuitive units, such as rotations or degrees.

For more information about `MotorVelocityControllerDeadBand`, visit our MotorVelocityController API Guide

| Device In Device # Identification

| error in (no error) error in can accept error information wired from VIs previously called.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| DeadBand The dead band value DCC1020_0 (ver: 103, 104) Velocity Controller: Default: 0 DCC1030_0 (ver: 104) Velocity Controller: Default: 0 DCC1120_0 (ver: 104, 105) Velocity Controller: Default: 0 DCC1130_0 (ver: 105) Velocity Controller: Default: 0

| Device Out Same as Device In

| error out error out passes error or warning information out of a VI to be used by other VIs.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.