## Phidget Accelerometer.lvlib:AccelerometerSetDataInterval.vi

The `AccelerometerDataInterval` is the time that must elapse before the channel will fire another `Accelerometer_AccelerationChange` event.

- The data interval is bounded by `AccelerometerMinDataInterval` and `AccelerometerMaxDataInterval`.
- The timing between `Accelerometer_AccelerationChange` events can also be affected by the `AccelerometerAccelerationChangeTrigger`.

| Device In Device # Identification

| error in (no error) error in can accept error information wired from VIs previously called.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Interval The data interval value Units: milliseconds (ms) 1008_0 (ver: 101) 2-Axis Accelerometer: Min: 39 Max: 1000 Default: 273 1041_0 (ver: 200, 201, 202) 3-Axis Accelerometer: Min: 1 Max: 1000 Default: 256 1042_0 (ver: 300, 301, 302, 303) 3-Axis Accelerometer: Min: 4 Max: 1000 Default: 256 1043_0 (ver: 300, 301, 302) 3-Axis Accelerometer: Min: 1 Max: 1000 Default: 256 1043_1 (ver: 302) 3-Axis Accelerometer: Min: 1 Max: 1000 Default: 256 1044_0 (ver: 400, 401, 402, 403) 3-Axis Accelerometer: Min: 4 Max: 1000 Default: 256 1044_1 (ver: 500, 502) 3-Axis Accelerometer: Min: 4 Max: 1000 Default: 256 1044_1 (ver: 511) 3-Axis Accelerometer: Min: 4 Max: 1000 Default: 256 1049_0 (ver: 100, 101, 102) 3-Axis Accelerometer: Min: 1 Max: 1000 Default: 256 1053_0 (ver: 300, 301, 302) 2-Axis Accelerometer: Min: 16 Max: 1000 Default: 256 1056_0 (ver: 100, 101, 102) 3-Axis Accelerometer: Min: 4 Max: 1000 Default: 256 1056_0 (ver: 200) 3-Axis Accelerometer: Min: 4 Max: 1000 Default: 256 1059_0 (ver: 400, 401) 3-Axis Accelerometer: Min: 16 Max: 1000 Default: 256 MOT0100_0 (ver: 100, 103) 3-Axis Accelerometer: Min: 4 Max: 60000 Default: 250 MOT0100_0 (ver: 100, 103) 3-Axis Accelerometer: Min: 4 Max: 60000 Default: 250 MOT0109_0 (ver: 112, 113, 115, 117) 3-Axis Accelerometer: Min: 4 Max: 1000 Default: 256 MOT0110_0 (ver: 100, 104, 110) 3-Axis Accelerometer: Min: 1 Max: 1000 Default: 250 MOT0110_0 (ver: 100, 104, 110) 3-Axis Accelerometer: Min: 1 Max: 1000 Default: 250 MOT1100_0 (ver: 201, 202) 3-Axis Accelerometer: Min: 10 Max: 60000 Default: 250 MOT1101_0 (ver: 112, 113) 3-Axis Accelerometer: Min: 20 Max: 60000 Default: 250 MOT1102_0 (ver: 210, 212, 213) 3-Axis Accelerometer: Min: 20 Max: 60000 Default: 250 MOT1102_1 (ver: 300, 301) 3-Axis Accelerometer: Min: 20 Max: 60000 Default: 250

| Device Out Same as Device In

| error out error out passes error or warning information out of a VI to be used by other VIs.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.