## Phidget Current Input.lvlib:CurrentInputGetCurrent.vi

The most recent current value that the channel has reported.

- This value will always be between `CurrentInputMinCurrent` and `CurrentInputMaxCurrent`.

| Device In Device # Identification

| error in (no error) error in can accept error information wired from VIs previously called.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Device Out Same as Device In

| error out error out passes error or warning information out of a VI to be used by other VIs.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Current The current value Units: amperes (A) 1061_0 (ver: 100) RC Servo Motor Current Sensor: Min: 0 Max: 5 1061_0 (ver: 200) RC Servo Motor Current Sensor: Min: 0 Max: 5 1061_1 (ver: 300, 301, 302, 303, 304) RC Servo Motor Current Sensor: Min: 0 Max: 5 1063_0 (ver: 100) Bipolar Stepper Current Sensor: Min: 0 Max: 2.492 1063_1 (ver: 100, 101) Bipolar Stepper Current Sensor: Min: 0 Max: 2.492 1064_0 (ver: 100, 101, 102) DC Motor Current Sensor: Min: -37.9 Max: 37.9 1064_1 (ver: 102) DC Motor Current Sensor: Min: -37.9 Max: 37.9 1065_0 (ver: 100, 101) DC Motor Current Sensor: Min: -80 Max: 80 1065_1 (ver: 100, 101) DC Motor Current Sensor: Min: -80 Max: 80 1066_0 (ver: 100) RC Servo Motor Current Sensor: Min: 0 Max: 5 1066_1 (ver: 100, 101) RC Servo Motor Current Sensor: Min: 0 Max: 5 DAQ1400_0 (ver: 112) Current Input: Min: 0.0005 Max: 0.02 DAQ1400_0 (ver: 120, 121) Current Input: Min: 0.0005 Max: 0.02 DAQ1400_0 (ver: 130) Current Input: Min: 0.0005 Max: 0.02 DCC1000_0 (ver: 115) Current Sensor: Min: -25 Max: 25 DCC1000_0 (ver: 204, 205, 206) Current Sensor: Min: -25 Max: 25 DCC1000_0 (ver: 210, 211, 220) Current Sensor: Min: -25 Max: 25 DCC1020_0 (ver: 103, 104) Current Sensor: Min: -120 Max: 120 DCC1030_0 (ver: 104) Current Sensor: Min: -120 Max: 120 DCC1120_0 (ver: 104, 105) Current Sensor: Min: -120 Max: 120 DCC1130_0 (ver: 105) Current Sensor: Min: -120 Max: 120 LED0100_0 (ver: 101) Current Input: Min: 0 Max: 4 LED0100_0 (ver: 101) Current Input: Min: 0 Max: 4 VCP1100_0 (ver: 101, 102) Current Input: Min: -30 Max: 30