## Phidget Digital Output.lvlib:DigitalOutputStart.vi

Opens and initializes a Phidget Digital Output

| error in (no error) error in can accept error information wired from VIs previously called.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Device Info Information required to specify which Phidget to open

| Serial Number The device serial number

| Channel The channel index

| Port The hub port index

| IsHubPort The hub port mode (True if the channel is a hub port itself)

| Connection Selects whether to look for a Phidget on the Local machine, over a Remote network, or both (No Preference)

| LED Current Limit The current limit value Units: amperes (A) 1030_0 (ver: 100, 101, 200, 201, 202) LED Driver: Min: 0.03 Max: 0.03 Default: 0.03 1031_0 (ver: 100, 101) LED Driver: Min: 0 Max: 0.08 Default: 0.02 1032_0 (ver: 200, 201) LED Driver: Min: 0 Max: 0.08 Default: 0.02 LED1000_0 (ver: 104, 105) LED Driver: Min: 0 Max: 0.04 Default: 0.02

| LEDForwardVoltage The forward voltage value
Enumeration Values
Name | Value | Supported Devices
--- | --- | ---
1030_0 v100 v101 v200 v201 v202 | 1031_0 v100 v101 | 1032_0 v200 v201 | LED1000_0 v104 v105
LED_FORWARD_VOLTAGE_1_7V | 1 | X | ✓ | ✓ | X
LED_FORWARD_VOLTAGE_2_75V | 2 | X | ✓ | ✓ | X
LED_FORWARD_VOLTAGE_3_2V | 3 | ✓ | X | X | ✓
LED_FORWARD_VOLTAGE_3_9V | 4 | X | ✓ | ✓ | X
LED_FORWARD_VOLTAGE_4_0V | 5 | X | X | X | ✓
LED_FORWARD_VOLTAGE_4_8V | 6 | X | X | X | ✓
LED_FORWARD_VOLTAGE_5_0V | 7 | X | ✓ | ✓ | X
LED_FORWARD_VOLTAGE_5_6V | 8 | X | X | X | ✓
1030_0 (ver: 100, 101, 200, 201, 202) LED Driver: Default: LED_FORWARD_VOLTAGE_3_2V 1031_0 (ver: 100, 101) LED Driver: Default: LED_FORWARD_VOLTAGE_2_75V 1032_0 (ver: 200, 201) LED Driver: Default: LED_FORWARD_VOLTAGE_2_75V LED1000_0 (ver: 104, 105) LED Driver: Default: LED_FORWARD_VOLTAGE_3_2V

| Timeout (mSec) Timeout in milliseconds

| Attached? Returns TRUE is the device successfully attached, or FALSE otherwise

| error out error out passes error or warning information out of a VI to be used by other VIs.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Phidget ID Device # Identification

| Serial Number Return The device serial number