## Phidget PH Sensor.lvlib:PHSensorEventExe.vi

The most recent pH value the channel has measured will be reported in this event, which occurs when the `PHSensorDataInterval` has elapsed.

- If a `PHSensorPHChangeTrigger` has been set to a non-zero value, the `PHSensor_PHChange` event will not occur until the pH has changed by at least the `PHSensorPHChangeTrigger` value.

Device Support:

1058_0 (ver: 100, 101) PH Input : Supported

ADP1000_0 (ver: 104, 105) PH Sensor Input : Supported

| error in (no error) error in can accept error information wired from VIs previously called.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Devices In A list of devices registered for the same type of event

| Device In Device # Identification

| Event Registration Refnum In Event # Identification

| error out error out passes error or warning information out of a VI to be used by other VIs.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error out indicator on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error out indicator on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source string describes the origin of the error or warning. Right-click the error out indicator on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Event? Returns TRUE if the event has executed, or FALSE otherwise.

| Devices Out Same as Devices In

| Device Out Same as Device In

| Index The index of the device that triggered the event within the Devices In array.

| pH The current pH

| phid Device # Identification of the device that triggered the event.

| Event Registration Refnum Out Same as Event Registration Refnum In