## Phidget Stepper.lvlib:StepperSetTargetPosition.vi

The controller will move the motor toward the `StepperTargetPosition` when `StepperEngaged` is TRUE.

- `StepperTargetPosition` is only used when `CONTROL_MODE_STEP` is selected.
- Use the `StepperRescaleFactor` to convert the units of this property into more intuitive units such as rotations or degrees.

For more information about `StepperTargetPosition`, visit our Stepper API Guide.

| Device In Device # Identification

| error in (no error) error in can accept error information wired from VIs previously called.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Target Position The position value 1062_0 (ver: 101) Unipolar Stepper Controller: Default: 0 1062_1 (ver: 101, 102) Unipolar Stepper Controller: Default: 0 1063_0 (ver: 100) Bipolar Stepper Controller: Default: 0 1063_1 (ver: 100, 101) Bipolar Stepper Controller: Default: 0 1067_0 (ver: 200, 201, 202, 203, 204, 205, 206) Bipolar Stepper Controller: Default: 0 STC1000_0 (ver: 100, 101) Bipolar Stepper Controller: Must be set STC1000_0 (ver: 110, 111, 112, 113, 114, 121, 122) Bipolar Stepper Controller: Must be set STC1001_0 (ver: 100, 101) Bipolar Stepper Controller: Must be set STC1001_0 (ver: 110, 111, 112, 113, 114, 115, 121, 122) Bipolar Stepper Controller: Must be set STC1002_0 (ver: 101, 102) Bipolar Stepper Controller: Must be set STC1002_0 (ver: 110, 111, 112, 113, 114, 121, 122) Bipolar Stepper Controller: Must be set STC1003_0 (ver: 100, 101) Bipolar Stepper Controller: Must be set STC1003_0 (ver: 110, 111, 112, 113, 114, 121, 122) Bipolar Stepper Controller: Must be set STC1003_1 (ver: 201, 221, 222) Bipolar Stepper Controller: Must be set STC1005_0 (ver: 100) Bipolar Stepper Controller: Must be set STC1005_0 (ver: 110, 111) Bipolar Stepper Controller: Must be set

| Device Out Same as Device In

| error out error out passes error or warning information out of a VI to be used by other VIs.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.