## Phidget Sound Sensor.lvlib:SoundSensorEventExe.vi

The most recent SPL values the channel has measured will be reported in this event, which occurs when the `SoundSensorDataInterval` has elapsed.

- If a `SoundSensorSPLChangeTrigger` has been set to a non-zero value, the `SoundSensor_SPLChange` event will not occur until the `SoundSensordB` SPL value has changed by at least the `SoundSensorSPLChangeTrigger` value.
- The dB SPL value is calculated from the `SoundSensorOctaves` data.
- The dBA SPL value is calculated by applying a A-weighted filter to the `SoundSensorOctaves` data.
- The dBC SPL value is calculated by applying a C-weighted filter to the `SoundSensorOctaves` data.
- The following frequency bands are represented:

- octaves[0] = 31.5 Hz
- octaves[1] = 63 Hz
- octaves[2] = 125 Hz
- octaves[3] = 250 Hz
- octaves[4] = 500 Hz
- octaves[5] = 1 kHz
- octaves[6] = 2 kHz
- octaves[7] = 4 kHz
- octaves[8] = 8 kHz
- octaves[9] = 16 kHz

Device Support:

SND1000_0 (ver: 101, 102) Sound Sensor : Supported

SND1000_1 (ver: 102) Sound Sensor : Supported

| error in (no error) error in can accept error information wired from VIs previously called.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Devices In A list of devices registered for the same type of event

| Device In Device # Identification

| Event Registration Refnum In Event # Identification

| error out error out passes error or warning information out of a VI to be used by other VIs.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error out indicator on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error out indicator on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source string describes the origin of the error or warning. Right-click the error out indicator on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Event? Returns TRUE if the event has executed, or FALSE otherwise.

| Devices Out Same as Devices In

| Device Out Same as Device In

| Index The index of the device that triggered the event within the Devices In array.

| phid Device # Identification of the device that triggered the event.

| Event Registration Refnum Out Same as Event Registration Refnum In

| dB The dB value Units: sound pressure level (dB SPL) SND1000_0 (ver: 101, 102) Sound Sensor: Max: 102 SND1000_1 (ver: 102) Sound Sensor: Max: 102

| dBA The dBA value Units: sound pressure level (dB SPL) SND1000_0 (ver: 101, 102) Sound Sensor: SND1000_1 (ver: 102) Sound Sensor:

| dBC The dBC value Units: sound pressure level (dB SPL) SND1000_0 (ver: 101, 102) Sound Sensor: SND1000_1 (ver: 102) Sound Sensor:

| Octaves The octave values Units: sound pressure level (dB SPL) SND1000_0 (ver: 101, 102) Sound Sensor: SND1000_1 (ver: 102) Sound Sensor:

| Octave Octave