## Phidget Capacitive Touch.lvlib:CapacitiveTouch_TouchEventExe.vi

The most recent touch value the channel has measured will be reported in this event, which occurs when the `DataInterval` has elapsed.

- If a `TouchValueChangeTrigger` has been set to a non-zero value, the `Touch` event will not occur until the touch value has changed by at least the `TouchValueChangeTrigger` value.

Device Support:

1015_0 (ver: 500, 101, 102) Capacitive Slider Sensor : Supported

1016_0 (ver: 510, 101, 102) Capacitive Scroll Sensor : Supported

HIN1000_0 (ver: 104) Capacitive Touch Sensor : Supported

HIN1001_0 (ver: 103) Capacitive Touch Sensor : Supported

HIN1001_0 (ver: 103) Capacitive Scroll Wheel : Supported

| error in (no error) error in can accept error information wired from VIs previously called.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Devices In A list of devices registered for the same type of event

| Device In Device # Identification

| Event Registration Refnum In Event # Identification

| error out error out passes error or warning information out of a VI to be used by other VIs.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error out indicator on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error out indicator on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source string describes the origin of the error or warning. Right-click the error out indicator on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Event? Returns TRUE if the event has executed, or FALSE otherwise.

| Devices Out Same as Devices In

| Device Out Same as Device In

| phid Device # Identification of the device that triggered the event.

| Touch Value Value of the touch input axis.

| Index The index of the device that triggered the event within the Devices In array.

| Event Registration Refnum Out Same as Event Registration Refnum In