## Phidget Voltage Input.lvlib:VoltageInputSetDataInterval.vi

The minimum value that `DataInterval` can be set to.

| Device In Device # Identification

| error in (no error) error in can accept error information wired from VIs previously called.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Interval The data interval value Units: milliseconds (ms) 1011_0 (ver: 100, 101, 102, 103) Voltage Input: Min: 1 Max: 1000 Def: 256 1013_0 (ver: 800, 811, 820) Voltage Input: Min: 16 Max: 1000 Def: 256 1013_0 (ver: 821, 823) Voltage Input: Min: 16 Max: 1000 Def: 256 1018_0 (ver: 824, 825, 826) Voltage Input: Min: 16 Max: 1000 Def: 256 1018_1 (ver: 826) Voltage Input: Min: 16 Max: 1000 Def: 256 1019_0 (ver: 826) Voltage Input: Min: 16 Max: 1000 Def: 256 1070_0 (ver: 826) Voltage Input: Min: 16 Max: 1000 Def: 256 1010_0 (ver: 903, 904) Voltage Input: Min: 1 Max: 1000 Def: 256 1018_2 (ver: 900, 901, 902, 903, 904) Voltage Input: Min: 1 Max: 1000 Def: 256 1019_1 (ver: 903, 904) Voltage Input: Min: 1 Max: 1000 Def: 256 1072_0 (ver: 903) Voltage Input: Min: 1 Max: 1000 Def: 256 1073_0 (ver: 904) Voltage Input: Min: 1 Max: 1000 Def: 256 1048_0 (ver: 100, 101, 102) Voltage Input: Min: 32 Max: 60000 Def: 256 1051_0 (ver: 200, 201, 202) Voltage Input: Min: 32 Max: 60000 Def: 256 1051_1 (ver: 300) Voltage Input: Min: 32 Max: 60000 Def: 256 1051_2 (ver: 400, 401, 402) Voltage Input: Min: 32 Max: 60000 Def: 256 1058_0 (ver: 100, 101) Voltage Input: Min: 80 Max: 60000 Def: 256 1065_0 (ver: 100, 101) Voltage Input: Min: 8 Max: 60000 Def: 256 1065_1 (ver: 100, 101) Voltage Input: Min: 8 Max: 60000 Def: 256 1065_0 (ver: 100, 101) Supply Voltage Sensor: Min: 8 Max: 60000 Def: 256 1065_1 (ver: 100, 101) Supply Voltage Sensor: Min: 8 Max: 60000 Def: 256 1202_0 (ver: 100) Voltage Input: Min: 16 Max: 1000 Def: 256 1203_0 (ver: 100) Voltage Input: Min: 16 Max: 1000 Def: 256 1202_0 (ver: 120, 121) Voltage Input: Min: 16 Max: 1000 Def: 256 1202_1 (ver: 123, 124) Voltage Input: Min: 16 Max: 1000 Def: 256 1203_0 (ver: 120, 121) Voltage Input: Min: 16 Max: 1000 Def: 256 1203_1 (ver: 123, 124) Voltage Input: Min: 16 Max: 1000 Def: 256 1202_2 (ver: 200, 201, 202, 203, 204) Voltage Input: Min: 1 Max: 1000 Def: 256 1203_2 (ver: 200, 201, 202, 203, 204) Voltage Input: Min: 1 Max: 1000 Def: 256 HUB0000_0 (ver: 117, 118, 119) Voltage Input: Min: 1 Max: 60000 Def: 250 SBC3003_0 (ver: 101, 102) Voltage Input: Min: 1 Max: 60000 Def: 250 HUB0000_0 (ver: 121) Voltage Input: Min: 1 Max: 60000 Def: 250 HUB5000_0 (ver: 102) Voltage Input: Min: 1 Max: 60000 Def: 250 SBC3003_0 (ver: 108) Voltage Input: Min: 1 Max: 60000 Def: 250 ADP1000_0 (ver: 104) Voltage Input: Min: 50 Max: 60000 Def: 250 DAQ1000_0 (ver: 102, 103) Voltage Input: Min: 20 Max: 60000 Def: 250 DAQ1000_0 (ver: 110) Voltage Input: Min: 20 Max: 60000 Def: 250 DAQ1400_0 (ver: 112) Voltage Input: Min: 20 Max: 60000 Def: 250 SAF1000_0 (ver: 101, 102) Voltage Sensor: Min: 100 Max: 60000 Def: 250 TMP1100_0 (ver: 103, 105) Voltage Input: Min: 20 Max: 60000 Def: 250 TMP1101_0 (ver: 104, 106) Voltage Input: Min: 20 Max: 60000 Def: 250 VCP1000_0 (ver: 100) Voltage Input: Min: 100 Max: 60000 Def: 250 VCP1001_0 (ver: 100) Voltage Input: Min: 40 Max: 60000 Def: 250 VCP1002_0 (ver: 106) Voltage Input: Min: 40 Max: 60000 Def: 250

| Device Out Same as Device In

| error out error out passes error or warning information out of a VI to be used by other VIs.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.