## Phidget Encoder.lvlib:EncoderStart.vi

Opens and initializes a Phidget Encoder

| Change Trigger The amount of position change required for a change event to fire.

| Data Interval The interval between data events from the device channel

| error in (no error) error in can accept error information wired from VIs previously called.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Device Info Information required to specify which Phidget to open

| Serial Number The device serial number

| Channel The channel index

| Port The hub port index

| Connection Selects whether to look for a Phidget on the Local machine, over a Remote network, or both (No Preference)

| Timeout (mSec) Timeout in milliseconds

| Enabled The enabled value 1047_0 (ver: 100, 101, 102) Encoder Input: Def: 1 1047_1 (ver: 102, 103) Encoder Input: Def: 1 1052_0 (ver: 100) Encoder Input: Val: 1 1052_0 (ver: 101, 102, 103) Encoder Input: Val: 1 1052_0 (ver: 110, 111) Encoder Input: Val: 1 1057_0 (ver: 300, 301) Encoder Input: Val: 1 1057_1 (ver: 302) Encoder Input: Val: 1 1057_2 (ver: 302) Encoder Input: Val: 1 1065_0 (ver: 100, 101) Encoder Input: Val: 1 1065_1 (ver: 100, 101) Encoder Input: Val: 1 DCC1000_0 (ver: 115) Encoder Input: Val: 1 DCC1000_0 (ver: 204, 205, 206) Encoder Input: Val: 1 DCC1001_0 (ver: 114, 116, 117) Encoder Input: Val: 1 DCC1002_0 (ver: 100) Encoder Input: Val: 1 ENC1000_0 (ver: 101) Encoder Input: Def: 1 HIN1101_0 (ver: 101) Encoder Input: Def: 1

| IO Mode The IO mode value.
Enumeration Values
Name | Value | Supported Devices
--- | --- | ---
DCC1000_0 v115 | DCC1000_0 v204 v205 v206
| ENC1000_0 v101
ENCODER_IO_MODE_PUSH_PULL | 1 | ✓ | ✓ | ✓
ENCODER_IO_MODE_LINE_DRIVER_2K2 | 2 | ✓ | ✓ | ✓
ENCODER_IO_MODE_LINE_DRIVER_10K | 3 | ✓ | ✓ | ✓
ENCODER_IO_MODE_OPEN_COLLECTOR_2K2 | 4 | ✓ | ✓ | ✓
ENCODER_IO_MODE_OPEN_COLLECTOR_10K | 5 | ✓ | ✓ | ✓

1047_0 (ver: 100, 101, 102) Encoder Input: Unsupported

1047_1 (ver: 102, 103) Encoder Input: Unsupported

1052_0 (ver: 100) Encoder Input: Unsupported

1052_0 (ver: 101, 102, 103) Encoder Input: Unsupported

1052_0 (ver: 110, 111) Encoder Input: Unsupported

1057_0 (ver: 300, 301) Encoder Input: Unsupported

1057_1 (ver: 302) Encoder Input: Unsupported

1057_2 (ver: 302) Encoder Input: Unsupported

1065_0 (ver: 100, 101) Encoder Input: Unsupported

1065_1 (ver: 100, 101) Encoder Input: Unsupported

DCC1000_0 (ver: 115) Encoder Input: Val: ENCODER_IO_MODE_PUSH_PULL

DCC1000_0 (ver: 204, 205, 206) Encoder Input: Val: ENCODER_IO_MODE_PUSH_PULL

DCC1001_0 (ver: 114, 116, 117) Encoder Input: Unsupported

DCC1002_0 (ver: 100) Encoder Input: Unsupported

ENC1000_0 (ver: 101) Encoder Input: Def: ENCODER_IO_MODE_PUSH_PULL

HIN1101_0 (ver: 101) Encoder Input: Unsupported

| Attached? Returns TRUE is the device successfully attached, or FALSE otherwise

| error out error out passes error or warning information out of a VI to be used by other VIs.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Phidget ID Device # Identification

| Serial Number Return The device serial number