## Phidget Voltage Ratio Input.lvlib:VoltageRatioInputVoltageRatioEventExe.vi

The most recent voltage ratio value the channel has measured will be reported in this event, which occurs when the `DataInterval` has elapsed.

- If a `VoltageRatioChangeTrigger` has been set to a non-zero value, the `VoltageRatioChange` event will not occur until the voltage has changed by at least the `VoltageRatioChangeTrigger` value.
- If ${PROPERTY:SensorType} is supported and set to anything other then `SENSOR_TYPE_VOLTAGERATIO`, this event will not fire.

Device Support:

1011_0 (ver: 100, 101, 102, 103) Voltage Ratio Input : Supported

1013_0 (ver: 800, 811, 820) Voltage Ratio Input : Supported

1013_0 (ver: 821, 823) Voltage Ratio Input : Supported

1018_0 (ver: 824, 825, 826) Voltage Ratio Input : Supported

1018_1 (ver: 826) Voltage Ratio Input : Supported

1019_0 (ver: 826) Voltage Ratio Input : Supported

1070_0 (ver: 826) Voltage Ratio Input : Supported

1010_0 (ver: 903, 904) Voltage Ratio Input : Supported

1018_2 (ver: 900, 901, 902, 903, 904) Voltage Ratio Input : Supported

1019_1 (ver: 903, 904) Voltage Ratio Input : Supported

1072_0 (ver: 903) Voltage Ratio Input : Supported

1073_0 (ver: 904) Voltage Ratio Input : Supported

1046_0 (ver: 100, 101) Bridge Input : Supported

1046_0 (ver: 102) Bridge Input : Supported

1065_0 (ver: 100, 101) Voltage Ratio Input : Supported

1065_1 (ver: 100, 101) Voltage Ratio Input : Supported

1202_0 (ver: 100) Voltage Ratio Input : Supported

1203_0 (ver: 100) Voltage Ratio Input : Supported

1202_0 (ver: 120, 121) Voltage Ratio Input : Supported

1202_1 (ver: 123, 124) Voltage Ratio Input : Supported

1203_0 (ver: 120, 121) Voltage Ratio Input : Supported

1203_1 (ver: 123, 124) Voltage Ratio Input : Supported

1202_2 (ver: 200, 201, 202, 203, 204) Voltage Ratio Input : Supported

1203_2 (ver: 200, 201, 202, 203, 204) Voltage Ratio Input : Supported

HUB0000_0 (ver: 117, 118, 119) Voltage Ratio Input : Supported

HUB0000_0 (ver: 121) Voltage Ratio Input : Supported

HUB5000_0 (ver: 102) Voltage Ratio Input : Supported

SBC3003_0 (ver: 101, 102) Voltage Ratio Input : Supported

SBC3003_0 (ver: 108) Voltage Ratio Input : Supported

DAQ1000_0 (ver: 102, 103) Voltage Ratio Input : Supported

DAQ1000_0 (ver: 110) Voltage Ratio Input : Supported

DAQ1500_0 (ver: 104) Bridge Input : Supported

DCC1000_0 (ver: 115) Voltage Ratio : Supported

DCC1000_0 (ver: 204, 205, 206) Voltage Ratio : Supported

HIN1100_0 (ver: 104, 105) Thumbstick Axis : Supported

| error in (no error) error in can accept error information wired from VIs previously called.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Devices In A list of devices registered for the same type of event

| Device In Device # Identification

| Event Registration Refnum In Event # Identification

| error out error out passes error or warning information out of a VI to be used by other VIs.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error out indicator on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error out indicator on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source string describes the origin of the error or warning. Right-click the error out indicator on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Event? Returns TRUE if the event has executed, or FALSE otherwise.

| Devices Out Same as Devices In

| Device Out Same as Device In

| Index The index of the device that triggered the event within the Devices In array.

| VoltageRatio The voltage ratio

| phid Device # Identification of the device that triggered the event.

| Event Registration Refnum Out Same as Event Registration Refnum In