## Phidget Stepper.lvlib:StepperGetIsMoving.vi

`IsMoving` returns true while the controller is sending commands to the motor. Note: there is no feedback to the controller, so it does not know whether the motor shaft is actually moving or not.

| Device In Device # Identification

| error in (no error) error in can accept error information wired from VIs previously called.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Device Out Same as Device In

| error out error out passes error or warning information out of a VI to be used by other VIs.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Moving The moving state 1062_0 (ver: 101) Unipolar Stepper Controller: 1062_1 (ver: 101, 102) Unipolar Stepper Controller: 1063_0 (ver: 100) Bipolar Stepper Controller: 1063_1 (ver: 100, 101) Bipolar Stepper Controller: 1067_0 (ver: 200, 201) Bipolar Stepper Controller: STC1000_0 (ver: 100) Bipolar Stepper Controller: STC1001_0 (ver: 100) Bipolar Stepper Controller: STC1002_0 (ver: 101) Bipolar Stepper Controller: STC1003_0 (ver: 100) Bipolar Stepper Controller: