## Phidget LCD.lvlib:LCDSetSleeping.vi

The on/off state of `Sleeping`. Putting the device to sleep turns off the display and backlight in order to save power.

- The device will still take commands while asleep, and will wake up if the screen is flushed, or if the contrast or backlight are changed.
- When the device wakes up, it will return to its last known state, taking into account any changes that happened while asleep.

| Device In Device # Identification

| error in (no error) error in can accept error information wired from VIs previously called.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Sleeping The sleep status 1202_0 (ver: 100) Text LCD: Unsupported 1202_0 (ver: 120, 121) Text LCD: Unsupported 1202_1 (ver: 123, 124) Text LCD: Unsupported 1203_0 (ver: 100) Text LCD: Unsupported 1203_0 (ver: 120, 121) Text LCD: Unsupported 1203_1 (ver: 123, 124) Text LCD: Unsupported 1202_2 (ver: 200, 201, 202, 203, 204) Text LCD: Unsupported 1203_2 (ver: 200, 201, 202, 203, 204) Text LCD: Unsupported 1204_0 (ver: 100, 101) Text LCD: Unsupported 1215_0 (ver: 100, 101) Text LCD: Unsupported 1216_0 (ver: 100, 101) Text LCD: Unsupported 1217_0 (ver: 100, 101) Text LCD: Unsupported 1218_0 (ver: 100, 101) Text LCD: Unsupported 1219_0 (ver: 110, 111, 113) Text LCD: Unsupported 1220_0 (ver: 110, 111, 113) Text LCD: Unsupported 1221_0 (ver: 110, 111, 113) Text LCD: Unsupported 1222_0 (ver: 110, 111, 113) Text LCD: Unsupported LCD1100_0 (ver: 106, 107, 108) Graphic LCD: Val: 1

| Device Out Same as Device In

| error out error out passes error or warning information out of a VI to be used by other VIs.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.