## Phidget RC Servo.lvlib:RCServo_PositionChangeEventExe.vi

An event that occurs when the position changes on a RC servo motor.

Device Support:

1000_0 (ver: 200, 201) RC Servo Motor Controller : Supported

1000_0 (ver: 300, 312) RC Servo Motor Controller : Supported

1000_0 (ver: 313) RC Servo Motor Controller : Supported

1001_0 (ver: 200, 201) RC Servo Motor Controller : Supported

1001_0 (ver: 300, 302, 312) RC Servo Motor Controller : Supported

1001_0 (ver: 313) RC Servo Motor Controller : Supported

1001_0 (ver: 313, 400) RC Servo Motor Controller : Supported

1061_0 (ver: 100) RC Servo Motor Controller : Supported

1061_0 (ver: 200) RC Servo Motor Controller : Supported

1061_1 (ver: 300, 301, 302, 303, 304) RC Servo Motor Controller : Supported

RCC0004_0 (ver: 400) RC Servo Motor Controller : Supported

1066_0 (ver: 100) RC Servo Motor Controller : Supported

1066_1 (ver: 100, 101) RC Servo Motor Controller : Supported

RCC1000_0 (ver: 106) RC Servo Motor Controller : Unsupported

| error in (no error) error in can accept error information wired from VIs previously called.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Devices In A list of devices registered for the same type of event

| Device In Device # Identification

| Event Registration Refnum In Event # Identification

| error out error out passes error or warning information out of a VI to be used by other VIs.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error out indicator on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error out indicator on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source string describes the origin of the error or warning. Right-click the error out indicator on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Event? Returns TRUE if the event has executed, or FALSE otherwise.

| Devices Out Same as Devices In

| Device Out Same as Device In

| Index The index of the device that triggered the event within the Devices In array.

| Position The position value

| phid Device # Identification of the device that triggered the event.

| Event Registration Refnum Out Same as Event Registration Refnum In