## Phidget DC Motor.lvlib:DCMotorSetFanMode.vi

The `FanMode` dictates the operating condition of the fan.

- Choose between on, off, or automatic (based on temperature).
- If the `FanMode` is set to automatic, the fan will turn on when the temperature reaches 70°C and it will remain on until the temperature falls below 55°C.
- If the `FanMode` is off, the controller will still turn on the fan if the temperature reaches 85°C and it will remain on until it falls below 70°C.

| Device In Device # Identification

| error in (no error) error in can accept error information wired from VIs previously called.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Fan Mode The fan mode
Enumeration Values
Name | Value | Supported Devices
--- | --- | ---
DCC1000_0 v115 | DCC1000_0 v204 v205 v206
FAN_MODE_OFF | 1 | ✓ | ✓
FAN_MODE_ON | 2 | ✓ | ✓
FAN_MODE_AUTO | 3 | ✓ | ✓

1060_0 (ver: 100, 110) DC Motor Controller: Unsupported

1064_0 (ver: 100, 101, 102) DC Motor Controller: Unsupported

1064_1 (ver: 102) DC Motor Controller: Unsupported

1065_0 (ver: 100, 101) DC Motor Controller: Unsupported

1065_1 (ver: 100, 101) DC Motor Controller: Unsupported

DCC1000_0 (ver: 115) DC Motor Controller: Val: FAN_MODE_AUTO

DCC1000_0 (ver: 204, 205, 206) DC Motor Controller: Val: FAN_MODE_AUTO

DCC1001_0 (ver: 114, 116, 117) DC Motor Controller: Unsupported

DCC1002_0 (ver: 100) DC Motor Controller: Unsupported

DCC1003_0 (ver: 100) DC Motor Controller: Unsupported

| Device Out Same as Device In

| error out error out passes error or warning information out of a VI to be used by other VIs.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.