## Phidget Temperature Sensor.lvlib:TemperatureSetThermocoupleType.vi

The `ThermocoupleType` must correspond to the thermocouple type you are using in your application.

- If you are unsure which `ThermocoupleType` to use, visit the Thermocouple Primer for more information.

| Device In Device # Identification

| error in (no error) error in can accept error information wired from VIs previously called.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| ThermocoupleType The thermocouple type
Enumeration Values
Name | Value | Supported Devices
--- | --- | ---
1048_0 v100 v101 v102 | 1051_0 v100 | 1051_0 v200 v201 v202 | 1051_1 v300 | 1051_2 v400 v401 v402 | TMP1100_0 v103 v105 | TMP1101_0 v104 v106
THERMOCOUPLE_TYPE_J | 1 | ✓ | X | ✓ | ✓ | ✓ | ✓ | ✓
THERMOCOUPLE_TYPE_K | 2 | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓
THERMOCOUPLE_TYPE_E | 3 | ✓ | X | ✓ | ✓ | ✓ | ✓ | ✓
THERMOCOUPLE_TYPE_T | 4 | ✓ | X | ✓ | ✓ | ✓ | ✓ | ✓
1045_0 (ver: 100, 101) Temperature Sensor (IR): Unsupported 1045_1 (ver: 101) Temperature Sensor (IR): Unsupported 1045_0 (ver: 100, 101) Temperature Sensor (IC): Unsupported 1045_1 (ver: 101) Temperature Sensor (IC): Unsupported 1048_0 (ver: 100, 101, 102) Thermocouple Input: Def: THERMOCOUPLE_TYPE_K 1048_0 (ver: 100, 101, 102) Temperature Sensor (IC): Unsupported 1051_0 (ver: 100) Thermocouple Input: Val: THERMOCOUPLE_TYPE_K 1051_0 (ver: 100) Temperature Sensor (IC): Unsupported 1051_0 (ver: 200, 201, 202) Thermocouple Input: Def: THERMOCOUPLE_TYPE_K 1051_0 (ver: 200, 201, 202) Temperature Sensor (IC): Unsupported 1051_1 (ver: 300) Thermocouple Input: Def: THERMOCOUPLE_TYPE_K 1051_1 (ver: 300) Temperature Sensor (IC): Unsupported 1051_2 (ver: 400, 401, 402) Thermocouple Input: Def: THERMOCOUPLE_TYPE_K 1051_2 (ver: 400, 401, 402) Temperature Sensor (IC): Unsupported DCC1000_0 (ver: 115) Temperature Sensor: Unsupported DCC1000_0 (ver: 204, 205, 206) Temperature Sensor: Unsupported DCC1100_0 (ver: 113, 114) Temperature Sensor: Unsupported HUM1000_0 (ver: 104, 105) Temperature Sensor: Unsupported SAF1000_0 (ver: 101, 102) Temperature Sensor: Unsupported TMP1000_0 (ver: 105, 107) Temperature Sensor (IC): Unsupported TMP1100_0 (ver: 103, 105) Thermocouple Input: Def: THERMOCOUPLE_TYPE_K TMP1100_0 (ver: 103, 105) Temperature Sensor (IC): Unsupported TMP1101_0 (ver: 104, 106) Thermocouple Input: Def: THERMOCOUPLE_TYPE_K TMP1101_0 (ver: 104, 106) Temperature Sensor (IC): Unsupported TMP1200_0 (ver: 104, 105, 106) RTD input: Unsupported

| Device Out Same as Device In

| error out error out passes error or warning information out of a VI to be used by other VIs.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.