## Phidget Voltage Input.lvlib:VoltageInputSetSensorType.vi

We sell a variety of analog sensors that do not have their own API, they simply output a voltage that can be converted to a digital value using a specific formula. By matching the `SensorType` to your analog sensor, the correct formula will automatically be applied to data when you get the `SensorValue` or subscribe to the `SensorChange` event.

- The `SensorChange` event has its own change trigger associated with it: `SensorValueChangeTrigger`.
- Any data from getting the `SensorValue` or subscribing to the `SensorChange` event will have a `SensorUnit` associated with it.

Note: Unlike other properties such as `DeviceSerialNumber` or `Channel`, `SensorType` is set after the device is opened, not before.

| Device In Device # Identification

| error in (no error) error in can accept error information wired from VIs previously called.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Sensor Type The sensor type value
Enumeration Values
Name | Value | Supported Devices
--- | --- | ---
1011_0 v100 v101 v102 v103 | 1013_0 v800 v811 v820 | 1013_0 v821 v823 | 1018_0 v824 v825 v826 | 1018_1 v826 | 1019_0 v826 | 1070_0 v826 | 1010_0 v903 v904 | 1018_2 v900 v901 v902 v903 v904 | 1019_1 v903 v904 | 1072_0 v903 | 1073_0 v904 | 1065_0 v100 v101 | 1065_1 v100 v101 | 1202_0 v100 | 1203_0 v100 | 1202_0 v120 v121 | 1202_1 v123 v124 | 1203_0 v120 v121 | 1203_1 v123 v124 | 1202_2 v200 v201 v202 v203 v204 | 1203_2 v200 v201 v202 v203 v204 | HUB0000_0 v117 v118 v119 | SBC3003_0 v101 v102 | HUB0000_0 v121 | HUB5000_0 v102 | SBC3003_0 v108 | ADP1000_0 v104 | DAQ1000_0 v102 v103 | DAQ1000_0 v110
SENSOR_TYPE_VOLTAGE | 0 | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓
SENSOR_TYPE_1114 | 11140 | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | X | ✓ | ✓
SENSOR_TYPE_1117 | 11170 | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | X | ✓ | ✓
SENSOR_TYPE_1123 | 11230 | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | X | ✓ | ✓
SENSOR_TYPE_1127 | 11270 | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | X | ✓ | ✓
SENSOR_TYPE_1130_PH | 11301 | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | X | ✓ | ✓
SENSOR_TYPE_1130_ORP | 11302 | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | X | ✓ | ✓
SENSOR_TYPE_1132 | 11320 | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | X | ✓ | ✓
SENSOR_TYPE_1133 | 11330 | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | X | ✓ | ✓
SENSOR_TYPE_1135 | 11350 | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | X | ✓ | ✓
SENSOR_TYPE_1142 | 11420 | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | X | ✓ | ✓
SENSOR_TYPE_1143 | 11430 | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | X | ✓ | ✓
SENSOR_TYPE_3500 | 35000 | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | X | ✓ | ✓
SENSOR_TYPE_3501 | 35010 | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | X | ✓ | ✓
SENSOR_TYPE_3502 | 35020 | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | X | ✓ | ✓
SENSOR_TYPE_3503 | 35030 | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | X | ✓ | ✓
SENSOR_TYPE_3507 | 35070 | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | X | ✓ | ✓
SENSOR_TYPE_3508 | 35080 | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | X | ✓ | ✓
SENSOR_TYPE_3509 | 35090 | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | X | ✓ | ✓
SENSOR_TYPE_3510 | 35100 | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | X | ✓ | ✓
SENSOR_TYPE_3511 | 35110 | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | X | ✓ | ✓
SENSOR_TYPE_3512 | 35120 | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | X | ✓ | ✓
SENSOR_TYPE_3513 | 35130 | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | X | ✓ | ✓
SENSOR_TYPE_3514 | 35140 | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | X | ✓ | ✓
SENSOR_TYPE_3515 | 35150 | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | X | ✓ | ✓
SENSOR_TYPE_3516 | 35160 | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | X | ✓ | ✓
SENSOR_TYPE_3517 | 35170 | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | X | ✓ | ✓
SENSOR_TYPE_3518 | 35180 | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | X | ✓ | ✓
SENSOR_TYPE_3519 | 35190 | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | X | ✓ | ✓
SENSOR_TYPE_3584 | 35840 | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | X | ✓ | ✓
SENSOR_TYPE_3585 | 35850 | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | X | ✓ | ✓
SENSOR_TYPE_3586 | 35860 | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | X | ✓ | ✓
SENSOR_TYPE_3587 | 35870 | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | X | ✓ | ✓
SENSOR_TYPE_3588 | 35880 | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | X | ✓ | ✓
SENSOR_TYPE_3589 | 35890 | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | X | ✓ | ✓
1011_0 (ver: 100, 101, 102, 103) Voltage Input: Def: SENSOR_TYPE_VOLTAGE 1013_0 (ver: 800, 811, 820) Voltage Input: Def: SENSOR_TYPE_VOLTAGE 1013_0 (ver: 821, 823) Voltage Input: Def: SENSOR_TYPE_VOLTAGE 1018_0 (ver: 824, 825, 826) Voltage Input: Def: SENSOR_TYPE_VOLTAGE 1018_1 (ver: 826) Voltage Input: Def: SENSOR_TYPE_VOLTAGE 1019_0 (ver: 826) Voltage Input: Def: SENSOR_TYPE_VOLTAGE 1070_0 (ver: 826) Voltage Input: Def: SENSOR_TYPE_VOLTAGE 1010_0 (ver: 903, 904) Voltage Input: Def: SENSOR_TYPE_VOLTAGE 1018_2 (ver: 900, 901, 902, 903, 904) Voltage Input: Def: SENSOR_TYPE_VOLTAGE 1019_1 (ver: 903, 904) Voltage Input: Def: SENSOR_TYPE_VOLTAGE 1072_0 (ver: 903) Voltage Input: Def: SENSOR_TYPE_VOLTAGE 1073_0 (ver: 904) Voltage Input: Def: SENSOR_TYPE_VOLTAGE 1048_0 (ver: 100, 101, 102) Voltage Input: Unsupported 1051_0 (ver: 200, 201, 202) Voltage Input: Unsupported 1051_1 (ver: 300) Voltage Input: Unsupported 1051_2 (ver: 400, 401, 402) Voltage Input: Unsupported 1058_0 (ver: 100, 101) Voltage Input: Unsupported 1065_0 (ver: 100, 101) Voltage Input: Def: SENSOR_TYPE_VOLTAGE 1065_1 (ver: 100, 101) Voltage Input: Def: SENSOR_TYPE_VOLTAGE 1065_0 (ver: 100, 101) Supply Voltage Sensor: Unsupported 1065_1 (ver: 100, 101) Supply Voltage Sensor: Unsupported 1202_0 (ver: 100) Voltage Input: Def: SENSOR_TYPE_VOLTAGE 1203_0 (ver: 100) Voltage Input: Def: SENSOR_TYPE_VOLTAGE 1202_0 (ver: 120, 121) Voltage Input: Def: SENSOR_TYPE_VOLTAGE 1202_1 (ver: 123, 124) Voltage Input: Def: SENSOR_TYPE_VOLTAGE 1203_0 (ver: 120, 121) Voltage Input: Def: SENSOR_TYPE_VOLTAGE 1203_1 (ver: 123, 124) Voltage Input: Def: SENSOR_TYPE_VOLTAGE 1202_2 (ver: 200, 201, 202, 203, 204) Voltage Input: Def: SENSOR_TYPE_VOLTAGE 1203_2 (ver: 200, 201, 202, 203, 204) Voltage Input: Def: SENSOR_TYPE_VOLTAGE HUB0000_0 (ver: 117, 118, 119) Voltage Input: Def: SENSOR_TYPE_VOLTAGE SBC3003_0 (ver: 101, 102) Voltage Input: Def: SENSOR_TYPE_VOLTAGE HUB0000_0 (ver: 121) Voltage Input: Def: SENSOR_TYPE_VOLTAGE HUB5000_0 (ver: 102) Voltage Input: Def: SENSOR_TYPE_VOLTAGE SBC3003_0 (ver: 108) Voltage Input: Def: SENSOR_TYPE_VOLTAGE ADP1000_0 (ver: 104) Voltage Input: Def: SENSOR_TYPE_VOLTAGE DAQ1000_0 (ver: 102, 103) Voltage Input: Def: SENSOR_TYPE_VOLTAGE DAQ1000_0 (ver: 110) Voltage Input: Def: SENSOR_TYPE_VOLTAGE DAQ1400_0 (ver: 112) Voltage Input: Unsupported SAF1000_0 (ver: 101, 102) Voltage Sensor: Unsupported TMP1100_0 (ver: 103, 105) Voltage Input: Unsupported TMP1101_0 (ver: 104, 106) Voltage Input: Unsupported VCP1000_0 (ver: 100) Voltage Input: Unsupported VCP1001_0 (ver: 100) Voltage Input: Unsupported VCP1002_0 (ver: 106) Voltage Input: Unsupported

| Device Out Same as Device In

| error out error out passes error or warning information out of a VI to be used by other VIs.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.