## Phidget LCD.lvlib:LCDSetScreenSize.vi

The size of the LCD screen attached to the channel.

| Device In Device # Identification

| error in (no error) error in can accept error information wired from VIs previously called.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Screen Size The screen size
Enumeration Values
Name | Value | Supported Devices
--- | --- | ---
1202_0 v100 | 1202_0 v120 v121 | 1202_1 v123 v124 | 1203_0 v100 | 1203_0 v120 v121 | 1203_1 v123 v124 | 1202_2 v200 v201 v202 v203 v204 | 1203_2 v200 v201 v202 v203 v204 | 1204_0 v100 v101 | 1215_0 v100 v101 | 1216_0 v100 v101 | 1217_0 v100 v101 | 1218_0 v100 v101 | 1219_0 v110 v111 v113 | 1220_0 v110 v111 v113 | 1221_0 v110 v111 v113 | 1222_0 v110 v111 v113 | LCD1100_0 v106 v107
SCREEN_SIZE_NONE | 1 | X | X | X | X | X | X | X | X | ✓ | X | X | X | X | X | X | X | X | X
SCREEN_SIZE_1x8 | 2 | X | X | X | X | X | X | X | X | ✓ | X | X | X | X | X | X | X | X | X
SCREEN_SIZE_2x8 | 3 | X | X | X | X | X | X | X | X | ✓ | X | X | X | X | X | X | X | X | X
SCREEN_SIZE_1x16 | 4 | X | X | X | X | X | X | X | X | ✓ | X | X | X | X | X | X | X | X | X
SCREEN_SIZE_2x16 | 5 | X | X | X | X | X | X | X | X | ✓ | X | X | X | X | X | X | X | X | X
SCREEN_SIZE_4x16 | 6 | X | X | X | X | X | X | X | X | ✓ | X | X | X | X | X | X | X | X | X
SCREEN_SIZE_2x20 | 7 | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | ✓ | X
SCREEN_SIZE_4x20 | 8 | X | X | X | X | X | X | X | X | ✓ | X | X | X | X | X | X | X | X | X
SCREEN_SIZE_2x24 | 9 | X | X | X | X | X | X | X | X | ✓ | X | X | X | X | X | X | X | X | X
SCREEN_SIZE_1x40 | 10 | X | X | X | X | X | X | X | X | ✓ | X | X | X | X | X | X | X | X | X
SCREEN_SIZE_2x40 | 11 | X | X | X | X | X | X | X | X | ✓ | X | X | X | X | X | X | X | X | X
SCREEN_SIZE_4x40 | 12 | X | X | X | X | X | X | X | X | ✓ | X | X | X | X | X | X | X | X | X
SCREEN_SIZE_64x128 | 13 | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | X | ✓
1202_0 (ver: 100) Text LCD: Val: SCREEN_SIZE_2x20 1202_0 (ver: 120, 121) Text LCD: Val: SCREEN_SIZE_2x20 1202_1 (ver: 123, 124) Text LCD: Val: SCREEN_SIZE_2x20 1203_0 (ver: 100) Text LCD: Val: SCREEN_SIZE_2x20 1203_0 (ver: 120, 121) Text LCD: Val: SCREEN_SIZE_2x20 1203_1 (ver: 123, 124) Text LCD: Val: SCREEN_SIZE_2x20 1202_2 (ver: 200, 201, 202, 203, 204) Text LCD: Val: SCREEN_SIZE_2x20 1203_2 (ver: 200, 201, 202, 203, 204) Text LCD: Val: SCREEN_SIZE_2x20 1204_0 (ver: 100, 101) Text LCD: 1215_0 (ver: 100, 101) Text LCD: Val: SCREEN_SIZE_2x20 1216_0 (ver: 100, 101) Text LCD: Val: SCREEN_SIZE_2x20 1217_0 (ver: 100, 101) Text LCD: Val: SCREEN_SIZE_2x20 1218_0 (ver: 100, 101) Text LCD: Val: SCREEN_SIZE_2x20 1219_0 (ver: 110, 111, 113) Text LCD: Val: SCREEN_SIZE_2x20 1220_0 (ver: 110, 111, 113) Text LCD: Val: SCREEN_SIZE_2x20 1221_0 (ver: 110, 111, 113) Text LCD: Val: SCREEN_SIZE_2x20 1222_0 (ver: 110, 111, 113) Text LCD: Val: SCREEN_SIZE_2x20 LCD1100_0 (ver: 106, 107) Graphic LCD: Val: SCREEN_SIZE_64x128

| Device Out Same as Device In

| error out error out passes error or warning information out of a VI to be used by other VIs.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.