## Phidget Encoder.lvlib:EncoderSetDataInterval.vi

The `DataInterval` is the time that must elapse before the channel will fire another `PositionChange` event.

- The data interval is bounded by `MinDataInterval` and `MaxDataInterval`.
- The timing between `PositionChange` events can also affected by the `PositionChangeTrigger`.

| Device In Device # Identification

| error in (no error) error in can accept error information wired from VIs previously called.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Interval The data interval value Units: milliseconds (ms) 1047_0 (ver: 100, 101, 102) Encoder Input: Min: 8 Max: 60000 Def: 256 1047_1 (ver: 102, 103) Encoder Input: Min: 8 Max: 60000 Def: 256 1052_0 (ver: 100) Encoder Input: Min: 16 Max: 1000 Def: 256 1052_0 (ver: 101, 102, 103) Encoder Input: Min: 16 Max: 1000 Def: 256 1052_0 (ver: 110, 111) Encoder Input: Min: 16 Max: 1000 Def: 256 1057_0 (ver: 300, 301) Encoder Input: Min: 8 Max: 1000 Def: 256 1057_1 (ver: 302) Encoder Input: Min: 8 Max: 1000 Def: 256 1057_2 (ver: 302) Encoder Input: Min: 8 Max: 1000 Def: 256 1065_0 (ver: 100, 101) Encoder Input: Min: 8 Max: 1000 Def: 256 1065_1 (ver: 100, 101) Encoder Input: Min: 8 Max: 1000 Def: 256 DCC1000_0 (ver: 115) Encoder Input: Min: 100 Max: 60000Val: 250 DCC1000_0 (ver: 204, 205, 206) Encoder Input: Min: 100 Max: 60000Val: 250 DCC1001_0 (ver: 114, 116, 117) Encoder Input: Min: 50 Max: 60000 Def: 250 DCC1002_0 (ver: 100) Encoder Input: Min: 50 Max: 60000 Def: 250 ENC1000_0 (ver: 101) Encoder Input: Min: 20 Max: 1000 Def: 250 HIN1101_0 (ver: 101) Encoder Input: Min: 20 Max: 1000 Def: 250

| Device Out Same as Device In

| error out error out passes error or warning information out of a VI to be used by other VIs.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.