## Phidget Stepper.lvlib:StepperSetEngaged.vi

When this property is true, the controller will supply power to the motor coils.

- The controller must be `Engaged` in order to move the Stepper motor, or have it hold position.

| Device In Device # Identification

| error in (no error) error in can accept error information wired from VIs previously called.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Engaged The engaged state 1062_0 (ver: 101) Unipolar Stepper Controller: Val: 0 1062_1 (ver: 101, 102) Unipolar Stepper Controller: Val: 0 1063_0 (ver: 100) Bipolar Stepper Controller: Val: 0 1063_1 (ver: 100, 101) Bipolar Stepper Controller: Val: 0 1067_0 (ver: 200, 201) Bipolar Stepper Controller: Val: 0 STC1000_0 (ver: 100) Bipolar Stepper Controller: Val: 0 STC1001_0 (ver: 100) Bipolar Stepper Controller: Val: 0 STC1002_0 (ver: 101) Bipolar Stepper Controller: Val: 0 STC1003_0 (ver: 100) Bipolar Stepper Controller: Val: 0

| Device Out Same as Device In

| error out error out passes error or warning information out of a VI to be used by other VIs.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.