## Phidget Frequency Counter.lvlib:FrequencyCounterStart.vi

Opens and initializes a Phidget Frequency Counter

| FrequencyCutoff Frequency at which 0 Hz is assumed.

| error in (no error) error in can accept error information wired from VIs previously called.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Device Info Information required to specify which Phidget to open

| Serial Number The device serial number

| Channel The channel index

| Port The hub port index

| Connection Selects whether to look for a Phidget on the Local machine, over a Remote network, or both (No Preference)

| Timeout (mSec) Timeout in milliseconds

| Filter Type The filter value
Enumeration Values
Name | Value | Supported Devices
--- | --- | ---
1054_0 v100 v101 | DAQ1400_0 v112
FILTER_TYPE_ZERO_CROSSING | 1 | ✓ | X
FILTER_TYPE_LOGIC_LEVEL | 2 | ✓ | ✓
1054_0 (ver: 100, 101) Frequency Input: Def: FILTER_TYPE_LOGIC_LEVEL DAQ1400_0 (ver: 112) Frequency Input: Val: FILTER_TYPE_LOGIC_LEVEL

| Power Supply The power supply value
Enumeration Values
Name | Value | Supported Devices
--- | --- | ---
DAQ1400_0 v112
POWER_SUPPLY_OFF | 1 | ✓
POWER_SUPPLY_12V | 2 | ✓
POWER_SUPPLY_24V | 3 | ✓
1054_0 (ver: 100, 101) Frequency Input: Unsupported DAQ1400_0 (ver: 112) Frequency Input: Def: POWER_SUPPLY_12V

| Input Mode The input mode value
Enumeration Values
Name | Value | Supported Devices
--- | --- | ---
DAQ1400_0 v112
INPUT_MODE_NPN | 1 | ✓
INPUT_MODE_PNP | 2 | ✓
1054_0 (ver: 100, 101) Frequency Input: Unsupported DAQ1400_0 (ver: 112) Frequency Input: Def: INPUT_MODE_NPN

| DataInterval The data interval value Units: milliseconds (ms) 1054_0 (ver: 100, 101) Frequency Input: Min: 32 Max: 60000 Def: 256 DAQ1400_0 (ver: 112) Frequency Input: Min: 20 Max: 60000 Def: 250

| Attached? Returns TRUE is the device successfully attached, or FALSE otherwise

| error out error out passes error or warning information out of a VI to be used by other VIs.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Phidget ID Device # Identification

| Serial Number Return The device serial number