## Phidget Digital Input.lvlib:DigitalInputEventExe.vi

This event will occur when the state of the digital input has changed.

- The value will either be 0 or 1 (true or false).

Device Support:

1011_0 (ver: 100, 101, 102, 103) Digital Input : Supported

1012_0 (ver: 600) Digital Input : Supported

1012_0 (ver: 601) Digital Input : Supported

1012_0 (ver: 602, 603, 604) Digital Input : Supported

1012_1 (ver: 605) Digital Input : Supported

1012_2 (ver: 605) Digital Input : Supported

1013_0 (ver: 800, 811, 820) Digital Input : Supported

1013_0 (ver: 821, 823) Digital Input : Supported

1018_0 (ver: 824, 825, 826) Digital Input : Supported

1018_1 (ver: 826) Digital Input : Supported

1019_0 (ver: 826) Digital Input : Supported

1070_0 (ver: 826) Digital Input : Supported

1010_0 (ver: 903, 904) Digital Input : Supported

1018_2 (ver: 900, 901, 902, 903, 904) Digital Input : Supported

1019_1 (ver: 903, 904) Digital Input : Supported

1072_0 (ver: 903) Digital Input : Supported

1073_0 (ver: 904) Digital Input : Supported

1047_0 (ver: 100, 101, 102) Digital Input : Supported

1047_1 (ver: 102, 103) Digital Input : Supported

1052_0 (ver: 100) Digital Input : Supported

1052_0 (ver: 101, 102, 103) Digital Input : Supported

1052_0 (ver: 110, 111) Digital Input : Supported

1060_0 (ver: 100, 110) Digital Input : Supported

1063_0 (ver: 100) Digital Input : Supported

1063_1 (ver: 100, 101) Digital Input : Supported

1065_0 (ver: 100, 101) Digital Input : Supported

1065_1 (ver: 100, 101) Digital Input : Supported

1202_0 (ver: 100) Digital Input : Supported

1203_0 (ver: 100) Digital Input : Supported

1202_0 (ver: 120, 121) Digital Input : Supported

1202_1 (ver: 123, 124) Digital Input : Supported

1203_0 (ver: 120, 121) Digital Input : Supported

1203_1 (ver: 123, 124) Digital Input : Supported

1202_2 (ver: 200, 201, 202, 203, 204) Digital Input : Supported

1203_2 (ver: 200, 201, 202, 203, 204) Digital Input : Supported

1219_0 (ver: 110, 111, 113) Digital Input : Supported

1220_0 (ver: 110, 111, 113) Digital Input : Supported

1221_0 (ver: 110, 111, 113) Digital Input : Supported

1222_0 (ver: 110, 111, 113) Digital Input : Supported

HUB0000_0 (ver: 117, 118, 119) Digital Input : Supported

HUB0000_0 (ver: 121) Digital Input : Supported

HUB5000_0 (ver: 102) Digital Input : Supported

SBC3003_0 (ver: 101, 102) Digital Input : Supported

SBC3003_0 (ver: 108) Digital Input : Supported

DAQ1200_0 (ver: 103) Digital Input : Supported

DAQ1300_0 (ver: 102) Digital Input Isolated : Supported

DAQ1301_0 (ver: 100) Digital Input Isolated : Supported

DAQ1400_0 (ver: 112) Digital Input : Supported

HIN1101_0 (ver: 101) Digital Input : Supported

HIN1100_0 (ver: 104, 105) Thumbstick Button : Supported

| error in (no error) error in can accept error information wired from VIs previously called.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Devices In A list of devices registered for the same type of event

| Device In Device # Identification

| Event Registration Refnum In Event # Identification

| error out error out passes error or warning information out of a VI to be used by other VIs.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error out indicator on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error out indicator on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source string describes the origin of the error or warning. Right-click the error out indicator on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Event? Returns TRUE if the event has executed, or FALSE otherwise.

| Devices Out Same as Devices In

| Device Out Same as Device In

| Index The index of the device that triggered the event within the Devices In array.

| State The state value

| phid Device # Identification of the device that triggered the event.

| State (Numeric) The state of the digital input as returned from the Phidget22 library. This can be 0 for FALSE, 1 for TRUE, or 2 for UNKNOWN.

| Event Registration Refnum Out Same as Event Registration Refnum In