## Phidget Capacitive Touch.lvlib:CapacitiveTouchStart.vi

Opens and initializes a Phidget Capacitive Touch

| Change Trigger The change trigger value 1015_0 (ver: 500, 101, 102) Capacitive Slider Sensor: Min: 0 Max: 1 Def: 0.005 1016_0 (ver: 510, 101, 102) Capacitive Scroll Sensor: Min: 0 Max: 1 Def: 0.005 HIN1000_0 (ver: 104) Capacitive Touch Sensor: Min: 0 Max: 1 Def: 0 HIN1001_0 (ver: 103) Capacitive Touch Sensor: Min: 0 Max: 0.5 Def: 0 HIN1001_0 (ver: 103) Capacitive Scroll Wheel: Min: 0 Max: 0.5 Def: 0

| Data Interval The data interval value Units: milliseconds (ms) 1015_0 (ver: 500, 101, 102) Capacitive Slider Sensor: Min: 60 Max: 1000 Def: 60 1016_0 (ver: 510, 101, 102) Capacitive Scroll Sensor: Min: 60 Max: 1000 Def: 60 HIN1000_0 (ver: 104) Capacitive Touch Sensor: Min: 25 Max: 1000 Def: 25 HIN1001_0 (ver: 103) Capacitive Touch Sensor: Min: 20 Max: 250 Def: 20 HIN1001_0 (ver: 103) Capacitive Scroll Wheel: Min: 20 Max: 250 Def: 20

| error in (no error) error in can accept error information wired from VIs previously called.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Device Info Information required to specify which Phidget to open

| Serial Number The device serial number

| Channel The channel index

| Port The hub port index

| Connection Selects whether to look for a Phidget on the Local machine, over a Remote network, or both (No Preference)

| Timeout (mSec) Timeout in milliseconds

| Attached? Returns TRUE is the device successfully attached, or FALSE otherwise

| error out error out passes error or warning information out of a VI to be used by other VIs.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Phidget ID Device # Identification

| Serial Number Return The device serial number