## Phidget Voltage Output.lvlib:VoltageOutputStart.vi

Opens and initializes a Phidget Voltage Output

| error in (no error) error in can accept error information wired from VIs previously called.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Device Info Information required to specify which Phidget to open

| Serial Number The device serial number

| Channel The channel index

| Port The hub port index

| Connection Selects whether to look for a Phidget on the Local machine, over a Remote network, or both (No Preference)

| Enabled The enabled value 1002_0 (ver: 100, 101) Voltage Output: Def: 1 OUT1000_0 (ver: 102) Voltage Output: Def: 1 OUT1001_0 (ver: 103) Voltage Output: Val: 1 OUT1002_0 (ver: 100) Voltage Output: Val: 1

| Voltage Output Range The output range value
Enumeration Values
Name | Value | Supported Devices
--- | --- | ---
1002_0 v100 v101 | OUT1001_0 v103
| OUT1002_0 v100
VOLTAGE_OUTPUT_RANGE_10V | 1 | ✓ | ✓ | ✓
VOLTAGE_OUTPUT_RANGE_5V | 2 | X | ✓ | ✓

1002_0 (ver: 100, 101) Voltage Output: Val: VOLTAGE_OUTPUT_RANGE_10V

OUT1000_0 (ver: 102) Voltage Output: Unsupported

OUT1001_0 (ver: 103) Voltage Output: Def: VOLTAGE_OUTPUT_RANGE_10V

OUT1002_0 (ver: 100) Voltage Output: Def: VOLTAGE_OUTPUT_RANGE_10V

| Timeout (mSec) Timeout in milliseconds

| Voltage The voltage value Units: volts (V) 1002_0 (ver: 100, 101) Voltage Output: Min: -10 Max: 10 Def: 0 OUT1000_0 (ver: 102) Voltage Output: Min: 0 Max: 4.2 Def: 0 OUT1001_0 (ver: 103) Voltage Output: Val: 0 OUT1002_0 (ver: 100) Voltage Output: Val: 0

| Attached? Returns TRUE is the device successfully attached, or FALSE otherwise

| error out error out passes error or warning information out of a VI to be used by other VIs.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Phidget ID Device # Identification

| Serial Number Return The device serial number