## Phidget Current Input.lvlib:CurrentInputSetDataInterval.vi

The `DataInterval` is the time that must elapse before the channel will fire another `CurrentChange` event.

- The data interval is bounded by `MinDataInterval` and `MaxDataInterval`.
- The timing between `CurrentChange` events can also affected by the `CurrentChangeTrigger`.

| Device In Device # Identification

| error in (no error) error in can accept error information wired from VIs previously called.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Interval The data interval value Units: milliseconds (ms) 1061_0 (ver: 100) RC Servo Motor Current Sensor: Min: 32 Max: 60000 Def: 256 1061_0 (ver: 200) RC Servo Motor Current Sensor: Min: 32 Max: 60000 Def: 256 1061_1 (ver: 300, 301, 302, 303, 304) RC Servo Motor Current Sensor: Min: 32 Max: 60000 Def: 256 1063_0 (ver: 100) Bipolar Stepper Current Sensor: Min: 8 Max: 60000 Def: 256 1063_1 (ver: 100, 101) Bipolar Stepper Current Sensor: Min: 8 Max: 60000 Def: 256 1064_0 (ver: 100, 101, 102) DC Motor Current Sensor: Min: 32 Max: 60000 Def: 256 1064_1 (ver: 102) DC Motor Current Sensor: Min: 32 Max: 60000 Def: 256 1065_0 (ver: 100, 101) DC Motor Current Sensor: Min: 8 Max: 60000 Def: 256 1065_1 (ver: 100, 101) DC Motor Current Sensor: Min: 8 Max: 60000 Def: 256 1066_0 (ver: 100) RC Servo Motor Current Sensor: Min: 32 Max: 60000 Def: 256 1066_1 (ver: 100, 101) RC Servo Motor Current Sensor: Min: 32 Max: 60000 Def: 256 DAQ1400_0 (ver: 112) Current Input: Min: 20 Max: 60000 Def: 250 VCP1100_0 (ver: 101) Current Input: Min: 20 Max: 60000 Def: 250 DCC1000_0 (ver: 115) Current Sensor: Min: 100 Max: 60000Val: 250 DCC1000_0 (ver: 204, 205, 206) Current Sensor: Min: 100 Max: 60000Val: 250

| Device Out Same as Device In

| error out error out passes error or warning information out of a VI to be used by other VIs.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.