## Phidget Digital Output.lvlib:DigitalOutputSetFrequency.vi

The `Frequency` parameter sets the PWM frequency for all frequency-settable PWM outputs on the board.

| Device In Device # Identification

| error in (no error) error in can accept error information wired from VIs previously called.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Frequency The PWM frequency Units: hertz (Hz) 1011_0 (ver: 100, 101, 102, 103) Digital Output: Unsupported 1012_0 (ver: 600) Digital Output: Unsupported 1012_0 (ver: 601) Digital Output: Unsupported 1012_0 (ver: 602, 603, 604) Digital Output: Unsupported 1012_1 (ver: 605) Digital Output: Unsupported 1012_2 (ver: 605) Digital Output: Unsupported 1013_0 (ver: 800, 811, 820) Digital Output: Unsupported 1013_0 (ver: 821, 823) Digital Output: Unsupported 1018_0 (ver: 824, 825, 826) Digital Output: Unsupported 1018_1 (ver: 826) Digital Output: Unsupported 1019_0 (ver: 826) Digital Output: Unsupported 1070_0 (ver: 826) Digital Output: Unsupported 1014_0 (ver: 700) Power Relay: Unsupported 1014_0 (ver: 704, 705, 706) Power Relay: Unsupported 1014_1 (ver: 707) Power Relay: Unsupported 1014_2 (ver: 707) Power Relay: Unsupported 1017_0 (ver: 100) Signal Relay: Unsupported 1017_1 (ver: 100) Signal Relay: Unsupported 1010_0 (ver: 903, 904) Digital Output: Unsupported 1018_2 (ver: 900, 901, 902, 903, 904) Digital Output: Unsupported 1019_1 (ver: 903, 904) Digital Output: Unsupported 1072_0 (ver: 903) Digital Output: Unsupported 1073_0 (ver: 904) Digital Output: Unsupported 1023_0 (ver: 200) Digital Output: Unsupported 1023_0 (ver: 200) LED Driver: Unsupported 1023_0 (ver: 200) Onboard LED: Unsupported 1023_0 (ver: 201, 202, 203, 204) Digital Output: Unsupported 1023_1 (ver: 205, 206) Digital Output: Unsupported 1023_0 (ver: 201, 202, 203, 204) LED Driver: Unsupported 1023_1 (ver: 205, 206) LED Driver: Unsupported 1023_0 (ver: 201, 202, 203, 204) Onboard LED: Unsupported 1023_1 (ver: 205, 206) Onboard LED: Unsupported 1024_0 (ver: 100, 101, 103) Digital Output: Unsupported 1024_0 (ver: 100, 101, 103) LED Driver: Unsupported 1024_0 (ver: 100, 101, 103) Onboard LED: Unsupported 1030_0 (ver: 100, 101, 200, 201, 202) LED Driver: Unsupported 1031_0 (ver: 100, 101) LED Driver: Unsupported 1032_0 (ver: 200, 201) LED Driver: Unsupported 1202_0 (ver: 100) Digital Output: Unsupported 1203_0 (ver: 100) Digital Output: Unsupported 1202_0 (ver: 120, 121) Digital Output: Unsupported 1202_1 (ver: 123, 124) Digital Output: Unsupported 1203_0 (ver: 120, 121) Digital Output: Unsupported 1203_1 (ver: 123, 124) Digital Output: Unsupported 1202_2 (ver: 200, 201, 202, 203, 204) Digital Output: Unsupported 1203_2 (ver: 200, 201, 202, 203, 204) Digital Output: Unsupported 1219_0 (ver: 110, 111, 113) Digital Output: Unsupported 1220_0 (ver: 110, 111, 113) Digital Output: Unsupported 1221_0 (ver: 110, 111, 113) Digital Output: Unsupported 1222_0 (ver: 110, 111, 113) Digital Output: Unsupported HUB0000_0 (ver: 117, 118, 119) Digital Output: Unsupported HUB0000_0 (ver: 121, 125, 126) Digital Output: Unsupported HUB5000_0 (ver: 102, 104, 105) Digital Output: Unsupported SBC3003_0 (ver: 101, 102) Digital Output: Unsupported SBC3003_0 (ver: 108, 109) Digital Output: Unsupported OUT1100_0 (ver: 100) Digital Output: Unsupported OUT1100_0 (ver: 110) Digital Output: Unsupported LED1000_0 (ver: 104) LED Driver: Unsupported REL1000_0 (ver: 101) Power Relay: Unsupported REL1000_0 (ver: 110) Power Relay: Unsupported REL1100_0 (ver: 100) Digital Output Isolated: Unsupported REL1100_0 (ver: 110) Digital Output Isolated: Unsupported REL1101_0 (ver: 102) Digital Output Isolated: Unsupported REL1101_0 (ver: 110) Digital Output Isolated: Unsupported

| Device Out Same as Device In

| error out error out passes error or warning information out of a VI to be used by other VIs.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.