## Phidget LCD.lvlib:LCDSaveFrameBuffer.vi

Writes the specified frame buffer to flash memory

- Use sparingly. The flash memory is only designed to be written to 10,000 times before it may become unusable. This method can only be called one time each time the channel is opened.

Device Support:

1202_0 (ver: 100) Text LCD : Unsupported

1202_0 (ver: 120, 121) Text LCD : Unsupported

1202_1 (ver: 123, 124) Text LCD : Unsupported

1203_0 (ver: 100) Text LCD : Unsupported

1203_0 (ver: 120, 121) Text LCD : Unsupported

1203_1 (ver: 123, 124) Text LCD : Unsupported

1202_2 (ver: 200, 201, 202, 203, 204) Text LCD : Unsupported

1203_2 (ver: 200, 201, 202, 203, 204) Text LCD : Unsupported

1204_0 (ver: 100, 101) Text LCD : Unsupported

1215_0 (ver: 100, 101) Text LCD : Unsupported

1216_0 (ver: 100, 101) Text LCD : Unsupported

1217_0 (ver: 100, 101) Text LCD : Unsupported

1218_0 (ver: 100, 101) Text LCD : Unsupported

1219_0 (ver: 110, 111, 113) Text LCD : Unsupported

1220_0 (ver: 110, 111, 113) Text LCD : Unsupported

1221_0 (ver: 110, 111, 113) Text LCD : Unsupported

1222_0 (ver: 110, 111, 113) Text LCD : Unsupported

LCD1100_0 (ver: 106, 107) Graphic LCD : Supported

| Device In Device # Identification

| error in (no error) error in can accept error information wired from VIs previously called.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| FrameBuffer The frame buffer to be saved

| Device Out Same as Device In

| error out error out passes error or warning information out of a VI to be used by other VIs.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.