## Phidget Encoder.lvlib:EncoderGetIndexPosition.vi

The most recent position of the index channel calculated by the Phidgets library.

- The index channel will usually pulse once per rotation.
- Setting the encoder position will move the index position the same amount so their relative position stays the same.
- Index position is tracked locally as the last position at which the index was triggered. Setting position will only affect the local copy of the index position value. This means that index positions seen by multiple network applications may not agree.

| Device In Device # Identification

| error in (no error) error in can accept error information wired from VIs previously called.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Device Out Same as Device In

| error out error out passes error or warning information out of a VI to be used by other VIs.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Index Pos The index position value 1047_0 (ver: 100, 101, 102) Encoder Input: Val: 0 1047_1 (ver: 102, 103) Encoder Input: Val: 0 1052_0 (ver: 100) Encoder Input: Unsupported 1052_0 (ver: 101, 102, 103) Encoder Input: Unsupported 1052_0 (ver: 110, 111) Encoder Input: Unsupported 1057_0 (ver: 300, 301) Encoder Input: Unsupported 1057_1 (ver: 302) Encoder Input: Unsupported 1057_2 (ver: 302) Encoder Input: Unsupported 1065_0 (ver: 100, 101) Encoder Input: Val: 0 1065_1 (ver: 100, 101) Encoder Input: Val: 0 DCC1000_0 (ver: 115) Encoder Input: Def: 0 DCC1000_0 (ver: 204, 205, 206) Encoder Input: Def: 0 DCC1001_0 (ver: 114, 116, 117) Encoder Input: Def: 0 DCC1002_0 (ver: 100) Encoder Input: Def: 0 ENC1000_0 (ver: 101) Encoder Input: Val: 0 HIN1101_0 (ver: 101) Encoder Input: Unsupported