## Phidget DC Motor.lvlib:DCMotorSetDataInterval.vi

The `DataInterval` is the time that must elapse before the controller will fire another `VelocityUpdate`/`BrakingStrengthChange` event.

- The data interval is bounded by `MinDataInterval` and `MaxDataInterval`.
- Note: `BrakingStrengthChange` events will only fire if a change in braking has occurred.

| Device In Device # Identification

| error in (no error) error in can accept error information wired from VIs previously called.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Interval The data interval value Units: milliseconds (ms) 1060_0 (ver: 100, 110) DC Motor Controller: Min: 64 Max: 60000 Def: 256 1064_0 (ver: 100, 101, 102) DC Motor Controller: Min: 32 Max: 60000 Def: 256 1064_1 (ver: 102) DC Motor Controller: Min: 32 Max: 60000 Def: 256 1065_0 (ver: 100, 101) DC Motor Controller: Min: 8 Max: 60000 Def: 256 1065_1 (ver: 100, 101) DC Motor Controller: Min: 8 Max: 60000 Def: 256 DCC1000_0 (ver: 115) DC Motor Controller: Min: 100 Max: 60000Val: 250 DCC1000_0 (ver: 204, 205, 206) DC Motor Controller: Min: 100 Max: 60000Val: 250 DCC1001_0 (ver: 114, 116, 117) DC Motor Controller: Min: 100 Max: 60000 Def: 250 DCC1002_0 (ver: 100) DC Motor Controller: Min: 100 Max: 60000 Def: 250 DCC1003_0 (ver: 100) DC Motor Controller: Min: 100 Max: 60000 Def: 250

| Device Out Same as Device In

| error out error out passes error or warning information out of a VI to be used by other VIs.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.