## Phidget Digital Output.lvlib:DigitalOutputResetFailsafe.vi

Resets the failsafe timer, if one has been set. See `EnableFailsafe` for details.

This function will fail if no failsafe timer has been set for the channel.

Device Support:

1011_0 (ver: 100, 101, 102, 103) Digital Output : Unsupported

1012_0 (ver: 600) Digital Output : Unsupported

1012_0 (ver: 601) Digital Output : Unsupported

1012_0 (ver: 602, 603, 604) Digital Output : Unsupported

1012_1 (ver: 605) Digital Output : Unsupported

1012_2 (ver: 605) Digital Output : Unsupported

1013_0 (ver: 800, 811, 820) Digital Output : Unsupported

1013_0 (ver: 821, 823) Digital Output : Unsupported

1018_0 (ver: 824, 825, 826) Digital Output : Unsupported

1018_1 (ver: 826) Digital Output : Unsupported

1019_0 (ver: 826) Digital Output : Unsupported

1070_0 (ver: 826) Digital Output : Unsupported

1014_0 (ver: 700) Power Relay : Unsupported

1014_0 (ver: 704, 705, 706) Power Relay : Unsupported

1014_1 (ver: 707) Power Relay : Unsupported

1014_2 (ver: 707) Power Relay : Unsupported

1017_0 (ver: 100) Signal Relay : Unsupported

1017_1 (ver: 100) Signal Relay : Unsupported

1010_0 (ver: 903, 904) Digital Output : Unsupported

1018_2 (ver: 900, 901, 902, 903, 904) Digital Output : Unsupported

1019_1 (ver: 903, 904) Digital Output : Unsupported

1072_0 (ver: 903) Digital Output : Unsupported

1073_0 (ver: 904) Digital Output : Unsupported

1023_0 (ver: 200) Digital Output : Unsupported

1023_0 (ver: 200) LED Driver : Unsupported

1023_0 (ver: 200) Onboard LED : Unsupported

1023_0 (ver: 201, 202, 203, 204) Digital Output : Unsupported

1023_1 (ver: 205, 206) Digital Output : Unsupported

1023_0 (ver: 201, 202, 203, 204) LED Driver : Unsupported

1023_1 (ver: 205, 206) LED Driver : Unsupported

1023_0 (ver: 201, 202, 203, 204) Onboard LED : Unsupported

1023_1 (ver: 205, 206) Onboard LED : Unsupported

1024_0 (ver: 100, 101, 103) Digital Output : Unsupported

1024_0 (ver: 100, 101, 103) LED Driver : Unsupported

1024_0 (ver: 100, 101, 103) Onboard LED : Unsupported

1030_0 (ver: 100, 101, 200, 201, 202) LED Driver : Unsupported

1031_0 (ver: 100, 101) LED Driver : Unsupported

1032_0 (ver: 200, 201) LED Driver : Unsupported

1202_0 (ver: 100) Digital Output : Unsupported

1203_0 (ver: 100) Digital Output : Unsupported

1202_0 (ver: 120, 121) Digital Output : Unsupported

1202_1 (ver: 123, 124) Digital Output : Unsupported

1203_0 (ver: 120, 121) Digital Output : Unsupported

1203_1 (ver: 123, 124) Digital Output : Unsupported

1202_2 (ver: 200, 201, 202, 203, 204) Digital Output : Unsupported

1203_2 (ver: 200, 201, 202, 203, 204) Digital Output : Unsupported

1219_0 (ver: 110, 111, 113) Digital Output : Unsupported

1220_0 (ver: 110, 111, 113) Digital Output : Unsupported

1221_0 (ver: 110, 111, 113) Digital Output : Unsupported

1222_0 (ver: 110, 111, 113) Digital Output : Unsupported

HUB0000_0 (ver: 117, 118, 119) Digital Output : Unsupported

HUB0000_0 (ver: 121) Digital Output : Unsupported

HUB5000_0 (ver: 102) Digital Output : Unsupported

SBC3003_0 (ver: 101, 102) Digital Output : Unsupported

SBC3003_0 (ver: 108) Digital Output : Unsupported

OUT1100_0 (ver: 100) Digital Output : Unsupported

OUT1100_0 (ver: 110) Digital Output : Supported

LED1000_0 (ver: 104) LED Driver : Unsupported

REL1000_0 (ver: 101) Power Relay : Unsupported

REL1000_0 (ver: 110) Power Relay : Supported

REL1100_0 (ver: 100) Digital Output Isolated : Unsupported

REL1100_0 (ver: 110) Digital Output Isolated : Supported

REL1101_0 (ver: 102) Digital Output Isolated : Unsupported

| Device In Device # Identification

| error in (no error) error in can accept error information wired from VIs previously called.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Device Out Same as Device In

| error out error out passes error or warning information out of a VI to be used by other VIs.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.