## Phidget BLDC Motor.lvlib:BLDCMotorSetAcceleration.vi

The rate at which the controller can change the motor's `Velocity`.

- The acceleration is bounded by `MinAccleration` and `MaxAcceleration`

  | Device In Device # Identification

  | error in (no error) error in can accept error information wired from VIs previously called.

  | status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

  | code code is the error or warning code. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

  | source source describes the origin of the error or warning. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

  | Acceleration The acceleration value Units: duty cycle per second (duty cycle/s) DCC1100_0 (ver: 113, 114) Brushless DC Motor Controller: Min: 0.1 Max: 100 Def: 1

  | Device Out Same as Device In

  | error out error out passes error or warning information out of a VI to be used by other VIs.

  | status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

  | code code is the error or warning code. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

  | source source describes the origin of the error or warning. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.