## Phidget Voltage Ratio Input.lvlib:VoltageRatioInputSetBridgeEnabled.vi

Enable power to and data from the input by setting `BridgeEnabled` to true.

| Device In Device # Identification

| error in (no error) error in can accept error information wired from VIs previously called.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Bridge Enabled The enabled value 1011_0 (ver: 100, 101, 102, 103) Voltage Ratio Input: Unsupported 1013_0 (ver: 800, 811, 820) Voltage Ratio Input: Unsupported 1013_0 (ver: 821, 823) Voltage Ratio Input: Unsupported 1018_0 (ver: 824, 825, 826) Voltage Ratio Input: Unsupported 1018_1 (ver: 826) Voltage Ratio Input: Unsupported 1019_0 (ver: 826) Voltage Ratio Input: Unsupported 1070_0 (ver: 826) Voltage Ratio Input: Unsupported 1010_0 (ver: 903, 904) Voltage Ratio Input: Unsupported 1018_2 (ver: 900, 901, 902, 903, 904) Voltage Ratio Input: Unsupported 1019_1 (ver: 903, 904) Voltage Ratio Input: Unsupported 1072_0 (ver: 903) Voltage Ratio Input: Unsupported 1073_0 (ver: 904) Voltage Ratio Input: Unsupported 1046_0 (ver: 100, 101) Bridge Input: Def: 1 1046_0 (ver: 102) Bridge Input: Def: 1 1065_0 (ver: 100, 101) Voltage Ratio Input: Unsupported 1065_1 (ver: 100, 101) Voltage Ratio Input: Unsupported 1202_0 (ver: 100) Voltage Ratio Input: Unsupported 1203_0 (ver: 100) Voltage Ratio Input: Unsupported 1202_0 (ver: 120, 121) Voltage Ratio Input: Unsupported 1202_1 (ver: 123, 124) Voltage Ratio Input: Unsupported 1203_0 (ver: 120, 121) Voltage Ratio Input: Unsupported 1203_1 (ver: 123, 124) Voltage Ratio Input: Unsupported 1202_2 (ver: 200, 201, 202, 203, 204) Voltage Ratio Input: Unsupported 1203_2 (ver: 200, 201, 202, 203, 204) Voltage Ratio Input: Unsupported HUB0000_0 (ver: 117, 118, 119) Voltage Ratio Input: Unsupported HUB0000_0 (ver: 121) Voltage Ratio Input: Unsupported HUB5000_0 (ver: 102) Voltage Ratio Input: Unsupported SBC3003_0 (ver: 101, 102) Voltage Ratio Input: Unsupported SBC3003_0 (ver: 108) Voltage Ratio Input: Unsupported DAQ1000_0 (ver: 102, 103) Voltage Ratio Input: Unsupported DAQ1000_0 (ver: 110) Voltage Ratio Input: Unsupported DAQ1500_0 (ver: 104) Bridge Input: Def: 1 DCC1000_0 (ver: 115) Voltage Ratio: Unsupported DCC1000_0 (ver: 204, 205, 206) Voltage Ratio: Unsupported HIN1100_0 (ver: 104, 105) Thumbstick Axis: Unsupported

| Device Out Same as Device In

| error out error out passes error or warning information out of a VI to be used by other VIs.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.