## Phidget Frequency Counter.lvlib:FrequencyCounterSetPowerSupply.vi

Choose the power supply voltage.

- See your controller's User Guide for more information about how the `PowerSupply` can be utilized in your application.

| Device In Device # Identification

| error in (no error) error in can accept error information wired from VIs previously called.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Power Supply The power supply value
Enumeration Values
Name | Value | Supported Devices
--- | --- | ---
DAQ1400_0 v100
POWER_SUPPLY_OFF | 1 | ✓
POWER_SUPPLY_12V | 2 | ✓
POWER_SUPPLY_24V | 3 | ✓
1054_0 (ver: 100, 101) Frequency Input: Unsupported DAQ1400_0 (ver: 100) Frequency Input: Def: POWER_SUPPLY_12V

| Device Out Same as Device In

| error out error out passes error or warning information out of a VI to be used by other VIs.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.