## Phidget Distance Sensor.lvlib:DistanceSensorSetDataInterval.vi

The `DataInterval` is the time that must elapse before the controller will fire another event.

- The data interval is bounded by `MinDataInterval` and `MaxDataInterval`.
- The timing between events can also affected by the change trigger.

  | Device In Device # Identification

  | error in (no error) error in can accept error information wired from VIs previously called.

  | status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

  | code code is the error or warning code. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

  | source source describes the origin of the error or warning. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

  | Interval The data interval value Units: milliseconds (ms) DST1000_0 (ver: 100) Distance Sensor 200mm: Min: 100 Max: 60000 Def: 250 DST1200_0 (ver: 100) Sonar Distance Sensor: Min: 100 Max: 60000 Def: 250

  | Device Out Same as Device In

  | error out error out passes error or warning information out of a VI to be used by other VIs.

  | status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

  | code code is the error or warning code. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

  | source source describes the origin of the error or warning. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.