## Phidget Voltage Output.lvlib:VoltageOutputSetVoltage.vi

The voltage value that the controller will output.

- The `Voltage` value is bounded by `MinVoltage` and `MaxVoltage`.
- The voltage value will not be output until `Enabled` is set to true.

| Device In Device # Identification

| error in (no error) error in can accept error information wired from VIs previously called.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| Voltage The voltage value Units: volts (V) 1002_0 (ver: 100, 101) Voltage Output: Min: -10 Max: 10 Def: 0 OUT1000_0 (ver: 100) Voltage Output: Min: 0 Max: 4.2 Def: 0 OUT1001_0 (ver: 100) Voltage Output: Min: undefined Max: undefinedVal: 0 OUT1002_0 (ver: 100) Voltage Output: Min: undefined Max: undefinedVal: 0

| Device Out Same as Device In

| error out error out passes error or warning information out of a VI to be used by other VIs.

| status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| code code is the error or warning code. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

| source source describes the origin of the error or warning. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.