## Phidget Frequency Counter.lvlib:FrequencyCounterSetFrequencyCutoff.vi

The frequency at which zero hertz is assumed.

- This means any frequency at or below the `FrequencyCutoff` value will be reported as 0 Hz.

- This property is stored locally, so other users who have this Phidget open over a network connection won't see the effects of your selected cutoff.

  | Device In Device # Identification

  | error in (no error) error in can accept error information wired from VIs previously called.

  | status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

  | code code is the error or warning code. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

  | source source describes the origin of the error or warning. Right-click the error in control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

  | FrequencyCutoff The frequency cutoff value Units: hertz (Hz) 1054_0 (ver: 100, 101) Frequency Input: Min: 0.01 Max: 10Val: 1 DAQ1400_0 (ver: 112) Frequency Input: Min: 0.01 Max: 10 Def: 1 DAQ1400_0 (ver: 120, 121) Frequency Input: Min: 0.01 Max: 10 Def: 1

  | Device Out Same as Device In

  | error out error out passes error or warning information out of a VI to be used by other VIs.

  | status status is TRUE (X) if an error occurred or FALSE (checkmark) to indicate a warning or that no error occurred. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

  | code code is the error or warning code. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.

  | source source describes the origin of the error or warning. Right-click the error out control on the front panel and select Explain Error or Explain Warning from the shortcut menu for more information about the error.